	CA001
	COSHH ASSESSMENT
CONTROL OF SUBSTANCES HAZARDOUS TO HEALTH REGULATIONS 2002
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	GAS OIL (DIESEL)

	Hazardous Contents:
	Ethylhexyl Nitrate



	GENERAL RISKS & CONTROLS

	Classification (state the category of danger)

	[image: ]
	☐	Serious Health Hazard/Toxic
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	☐	Oxidising
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	☐	Gas Under Pressure
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	☒	Health Hazard/ Harmful/Irritant
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	☒	Flammable
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	☒	Acute Toxicity/ Carcinogen
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	☐	Corrosive
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	☐	Explosive
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	☒	Dangerous for the Environment

	Hazard Type

	☒	☐	☐	☐	☐	☐	☐	☐
	Gas
	Water
	Mist
	Fume
	Dust
	Liquid
	Solid
	Other

	Route of Exposure

	☒	☒	☒	☒	☐	

	Inhalation
	Skin
	Eyes
	Ingestion
	Other (state)
	

	

	Workplace Exposure Limits (WELs) please indicate n/a where not applicable
	
68mg Derived No Effect Level

	Storage & Handling
	Hazard Symptoms

	· Store in cool, well ventilated area. Do NOT remove warning labels.
· Keep container tightly closed / Open slowly in order to control possible pressure release.
· Empty drums should be drained and safely stored away from full drums before disposal.
· Store on bund 110% capacity of container, and impermeable ground. Keep stored away from possible impact.
· Store away from sources of heat and ignition.
· Use mechanical aids when moving/handling full, and empty drums.
	· Flammable liquid and vapour.
· May be fatal if swallowed and enters airways.
· Causes skin irritation. Causes eye irritation
· May cause damage to liver, kidneys and nervous system by repeated and prolonged inhalation.Toxic to aquatic life with long lasting effects.
· Harmful if ingested.
· Gases and vapours may contribute to a flammable atmosphere.

	Controls
	Remedial Actions

	· Keep away from heat, sparks, open flames, welding and hot surfaces
· Do not siphon by mouth
· Wear PPE to prevent skin and eye contact with liquid.
· Avoid breathing vapours or mists. Do not eat, drink or smoke when using this product.
· Keep in bund container 110% capacity of container, on impermeable ground.
· Wash hands or liquid-contacted skin thoroughly after handling
· Use only outdoors or in a well-ventilated area.
	· Eliminate all ignition sources.
· Stop leak if you are able to without risk.
· Prevent entry into waterways, sewers, basement, and confined spaces.
· Absorb or cover with dry earth, sand, or other non-combustible material.
· Use clean non-spark tools to collect absorbed materials.

	Disposal

	Hazardous Waste?
 ☒
	Skip
☐
	Other ☒
· Dispose of waste or residues in accordance with local authority.
· Recycle packaging where applicable.
· Do NOT burn substance.

	Return to Depot 
☒
	Return to Supplier
☐
	

	FIRST AID
[image: ]
	FIRE FIGHTING
[image: ]


	· Dry wipe exposed skin and cleanse with waterless hand cleaner, follow by washing with soapy water.
· If respiratory irritation, dizziness, nausea, or unconsciousness occurs, seek medical advice.
	· Flush thoroughly with water. If irritation occurs seek medical assistance.
· Seek immediate medical attention. Do NOT induce vomiting.
· Remove victim from further exposure.
	WATER
☒
	FOAM
☒
	POWDER
☒
	CO2
☒
	CHEMICAL
☐

	· 
	· 
	PRECAUTIONS:
Do NOT use solid water Jet, use mist spray. Avoid residual water run-off into drains.


	SITE SPECIFIC CONTROLS

	Work Activities Being Undertaken

	Fuelling of Plant & Equipment on site

	Exposure

	Number of Persons
	Frequency
	Duration
	Any specific training requirements?

	5-10
	Daily
	30 mins
	☐
	Personal Protective Equipment (PPE) Control Measures
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	☒	☐	☐	☐	☐	☐	☒	☐	☐
	Eye Protection
	Ear Protection
	Hard Hat
	Footwear
	Overalls
	Visor
	Gloves
	Face Mask
	Respirator

	
	
	
	
	
	
	
	
	

	Storage Requirements

	
LOCKED CAGE
	BUNDED CONTAINER
	PROTECTION
FROM WEATHER
	COSHH STORAGE ROOM
	
SEALED CONTAINER

	☐	☒	☐	☐	☐
	Waste Management

	SEGREGATED STORAGE
	SEALED CONTAINERS
	WASTE CARRIER DISPOSAL / RECYCLING LICENCE

	☐	☒	☐
	Risk Rating Following Control Measures

	LOW
	MEDIUM
	HIGH

	☒	☐	☐


	Site Specific RA Prepared by:
	Si King 
	Position:
	Contracts Director 

	
	
	Review Date:
	27/09/2023
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Mandatory Symbols
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MAND1 MAND2 MAND3 MAND4 MANDS MANDG MAND?
General Mandatory ~ Wear Hearing  Wear Eye Protection WearHead ~ Wear Foot Protection  Wear Protective  Wear Face Shield
Action Protection Protection Clothing
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MAND8 MAND10 MAND11 MAND12 MAND13 MAND14 MAND15
Wear Hair Net Wear Face Mask Wear Hand Wear Respiralory  Wear High Visibility ~ Pedestrian Route  Wear Safety Hamess
Protection Protection Clothing
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MAND16 MAND17 MAND18 MAND19 MAND20 MAND21 MAND23
Wash Your Hands Check Guard Use Adjustable Keep Locked Sound Hom Lift Correctly Wear Anti-Static
Guard Footwear

MAND24 MAND25 MAND26 MAND27 MAND28 MAND29 MAND30

Wear Laboratory ~ Wear Life Jacket UselitlerBin  Switch OffAfter Use  Wear Seatbelt Use Ladder Use Stairs
Coat

MAND36 MANDA0 MAND41 MAND42 MAND43 MAND44 MANDAS
ConnectAnEarth  Wear Protective  Referto Instruction  Disconnect From Use Handrail Disconnect Before  Use Barrier Cream
Terminal To The Apron Manual/Booklet Mains Supply Carrying Out

Ground Maintenance/Repair

e
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MAND46 MAND47
Use Footbridge  Wear Opaque Eye
Protection
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