	CA002
	COSHH ASSESSMENT
CONTROL OF SUBSTANCES HAZARDOUS TO HEALTH REGULATIONS 2002
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	Engine Oil

	Hazardous Contents:
	Zinc alkyldithiophosphate. Tetrapropenylphenol. 
Calcium long chain Alkyl phenate sulphide.



	GENERAL RISKS & CONTROLS

	Classification (state the category of danger)
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	☐	Serious Health Hazard/Toxic
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	☐	Oxidising
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	☐	Gas Under Pressure

	[image: ]
	☒	Health Hazard/ Harmful/Irritant
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	☒	Flammable
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	☒	Acute Toxicity/ Carcinogen
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	☐	Corrosive
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	☐	Explosive
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	☐	Dangerous for the Environment

	Hazard Type

	☐	☐	☐	☐	☐	☒	☐	☐
	Gas
	Water
	Mist
	Fume
	Dust
	Liquid
	Solid
	Other

	Route of Exposure

	☐	☒	☒	☒	☐	

	Inhalation
	Skin
	Eyes
	Ingestion
	Other (state)
	

	

	Workplace Exposure Limits (WELs) please indicate n/a where not applicable
	
N/A

	Storage & Handling
	Hazard Symptoms

	· Store in cool, well ventilated area, out of direct sunlight, and away from heat and ignition sources.
· Keep container tightly closed / Wash hands thoroughly after handling.
· Empty drums should be drained and safely stored away from full drums before disposal with labels intact.
· Keep on bund, on impermeable ground.
· Store away from possible impact.
· Use mechanical aids when handling full and empty drums.	


	· Ingestion may cause gastrointestinal irritation and diarrhoea, or death
· Used engine oil may contain hazardous components which have the potential to cause cancer.
· Prolonged or repeated contact with skin could lead to irritation and/or dermatitis.
· Contact with eyes may cause irritation.
· Inhalation may cause respiratory tract irritation.
· Toxic to aquatic life with long lasting effects.
· Spills create a slippery surface.

	Controls
	Remedial Actions

	· Do NOT siphon by mouth. Do NOT eat drink or smoke.
· Wear appropriate PPE to prevent contact.
· Wear protective overalls were necessary. Avoid prolonged contact and handle with care to prevent splash.
· Wear appropriate eye protection. Avoid contact with the eyes.
· Use outside in a well-ventilated area.
· Prevent entry into the environment, drains, sewers, water courses.
· Clear up any spillages using available spill kit absorbent material.

	· Soak up with inert absorbent material.
· Remove contaminated absorbent material for remediation or disposal in accordance with local authority.
· If spilled on water, contain using a boom, and collect by skimming or absorption.

	Disposal

	Hazardous Waste?
 ☒
	Skip
☐
	Other ☒
· Place used and contaminated materials in suitable containers.
· Dispose using licensed waste disposal company.
· Do NOT pressurise, cut, weld, braze, solder, drill, grind, heat.

	Return to Depot 
☐
	Return to Supplier
☐
	

	FIRST AID
[image: ]
	FIRE FIGHTING
[image: ]


	· If inhaled, remove to fresh air. If symptoms appear, get medical attention.
· Wash skin as soon as possible with soap water.
·  Change contaminated clothing immediately and launder before re-use. Get medical attention if irritation persist.
	· Wash out eyes immediately with water, remove any contact lenses. If irritation persists seek medical advice.
· Do not induce vomiting, unless instructed to by medical persons.
· Seek medical attention if internal irritation symptoms occur.
	WATER
☐
	FOAM
☒
	POWDER
☒
	CO2
☒
	CHEMICAL
☐

	· 
	· 
	PRECAUTIONS:



	SITE SPECIFIC CONTROLS (TO BE COMPLETED ON SITE)

	Work Activities Being Undertaken

	

	Exposure

	Number of Persons
	Frequency
	Duration
	Any specific training requirements?

	
	
	
	☐
	Personal Protective Equipment (PPE) Control Measures
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	☐	☐	☐	☐	☐	☐	☐	☐	☐
	Eye Protection
	Ear Protection
	Hard Hat
	Footwear
	Overalls
	Visor
	Gloves
	Face Mask
	Respirator

	
	
	
	
	
	
	
	
	

	Storage Requirements

	
LOCKED CAGE
	BUNDED CONTAINER
	PROTECTION
FROM WEATHER
	COSHH STORAGE ROOM
	
SEALED CONTAINER

	☐	☐	☐	☐	☐
	Waste Management

	SEGREGATED STORAGE
	SEALED CONTAINERS
	WASTE CARRIER DISPOSAL / RECYCLING LICENCE

	☐	☒	☐
	Risk Rating Following Control Measures

	LOW
	MEDIUM
	HIGH

	☐	☐	☒


	Site Specific RA Prepared by:
	Si King 
	Position:
	Contracts Director 

	
	
	Review Date:
	27/09/2023
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Mandatory Symbols
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MAND1 MAND2 MAND3 MAND4 MANDS MANDG MAND?
General Mandatory ~ Wear Hearing  Wear Eye Protection WearHead ~ Wear Foot Protection  Wear Protective  Wear Face Shield
Action Protection Protection Clothing
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MAND8 MAND10 MAND11 MAND12 MAND13 MAND14 MAND15
Wear Hair Net Wear Face Mask Wear Hand Wear Respiralory  Wear High Visibility ~ Pedestrian Route  Wear Safety Hamess
Protection Protection Clothing
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MAND16 MAND17 MAND18 MAND19 MAND20 MAND21 MAND23
Wash Your Hands Check Guard Use Adjustable Keep Locked Sound Hom Lift Correctly Wear Anti-Static
Guard Footwear

MAND24 MAND25 MAND26 MAND27 MAND28 MAND29 MAND30

Wear Laboratory ~ Wear Life Jacket UselitlerBin  Switch OffAfter Use  Wear Seatbelt Use Ladder Use Stairs
Coat

MAND36 MANDA0 MAND41 MAND42 MAND43 MAND44 MANDAS
ConnectAnEarth  Wear Protective  Referto Instruction  Disconnect From Use Handrail Disconnect Before  Use Barrier Cream
Terminal To The Apron Manual/Booklet Mains Supply Carrying Out

Ground Maintenance/Repair

e
@

MAND46 MAND47
Use Footbridge  Wear Opaque Eye
Protection
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