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	COSHH ASSESSMENT
CONTROL OF SUBSTANCES HAZARDOUS TO HEALTH REGULATIONS 2002
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	CONCRETE DUST

	Hazardous Contents:
	Crystalline silica.



	GENERAL RISKS & CONTROLS

	Classification (state the category of danger)
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	☒	Serious Health Hazard/Toxic
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	☐	Oxidising
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	☐	Gas Under Pressure
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	☒	Health Hazard/ Harmful/Irritant
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	☐	Flammable
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	☒	Acute Toxicity/ Carcinogen
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	☐	Corrosive
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	☐	Explosive
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	☐	Dangerous for the Environment

	Hazard Type

	☐	☐	☐	☐	☒	☐	☐	☐
	Gas
	Water
	Mist
	Fume
	Dust
	Liquid
	Solid
	Other

	Route of Exposure

	☒	☒	☒	☐	☐	

	Inhalation
	Skin
	Eyes
	Ingestion
	Other (state)
	

	

	Workplace Exposure Limits (WELs) please indicate n/a where not applicable
	10mg
8 hours

	Storage & Handling
	Hazard Symptoms

	· Ensure spoil heaps are frequently doused with water  suppression.
· Hot weather will increase the build-up of dust.
· Windy conditions will kick up settles dust into the atmosphere.
	· Cutting/breaking hard cement may eject fragments at high speed that could cause injury.
· Cutting/breaking will disperse dust into the atmosphere.
· Breathing in airborne dust over a prolonged period of time will increase the risk of silicosis and lung cancer
· Dust settling on surfaces may make them become slippery.

	Controls
	· Remedial Actions

	· Ensure cutting/breaking equipment are fitting with adequate protection, and suitable PPE is warn to protect against projectiles.
· Ensure good ventilation in confined areas, and use dust suppression methods such water dampening.
· Ensure adequate RPE is warn when dust is likely to occur.
· Ensure surfaces including roads, are appropriately maintained to ensure the build-up of surface dust does not affect users.
	· Stop the process creating the dust.
· Avoid breathing in dust, wear dust mask/respirator as per your face fit test certificate and googles.
· Ensure sufficient ventilation.
· Used dust suppression methods.
· Vacuum, or wet mod dust once settled.
· Use dust monitoring devises to ensure the atmosphere is at a suitable level.

	Disposal

	Hazardous Waste?
 ☐
	Skip
☒
	Other ☒
· Residual dust collected by a vacuum or from sweeping can be  taken with the crushed concrete.
·  Do NOT pour down drains, sewers, watercourses.
· Waste should be disposed in accordance with local and national waste disposal regulation.

	Return to Depot 
☐
	Return to Supplier
☐
	

	FIRST AID
[image: ]
	FIRE FIGHTING
[image: ]


	· Remove to fresh air, and seek medical attention if required.
· Remove contaminated cloths.
· Wash skin thoroughly with warm soap water. If irritation continues, seek medical advice.
	· Remove contact lenses, flush with clean water for 10 minutes, seek medical attention if irritation continues.
· If accidently swallowed, remove from exposure and seek medical advice.
	WATER
☒
	FOAM
☒
	POWDER
☒
	CO2
☒
	CHEMICAL
☒

	· 
	· 
	Is not flammable – Will not facilities combustion with other materials.


	SITE SPECIFIC CONTROLS (TO BE COMPLETED ON SITE)

	Work Activities Being Undertaken

	

	Exposure

	Number of Persons
	Frequency
	Duration
	Any specific training requirements?

	5 -10 
	Daily 
	8 Hours 

	☐
	Personal Protective Equipment (PPE) Control Measures

	[image: ]
	[image: ]
	[image: ]
	[image: ]
	[image: ]
	[image: ]
	[image: ]
	[image: ]
	[image: ]

	☒	☐	☒	☒	☐	☐	☒	☒	☐
	Eye Protection
	Ear Protection
	Hard Hat
	Footwear
	Overalls
	Visor
	Gloves
	Face Mask
	Respirator

	
	
	
	
	
	
	
	
	

	Storage Requirements

	
LOCKED CAGE
	BUNDED CONTAINER
	PROTECTION
FROM WEATHER
	COSHH STORAGE ROOM
	
SEALED CONTAINER

	☐	☐	☒	☐	☐
	Waste Management

	SEGREGATED STORAGE
	SEALED CONTAINERS
	WASTE CARRIER DISPOSAL / RECYCLING LICENCE

	☒	☒	☐
	Risk Rating Following Control Measures

	LOW
	MEDIUM
	HIGH

	☒	☐	☒


	Site Specific RA Prepared by:
	Si King 
	Position:
	Contracts Director  

	
	
	Review Date:
	27/09/2023
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Mandatory Symbols

&
@®

©
@
=

MAND1 MAND2 MAND3 MAND4 MANDS MANDG MAND?
General Mandatory ~ Wear Hearing  Wear Eye Protection WearHead ~ Wear Foot Protection  Wear Protective  Wear Face Shield
Action Protection Protection Clothing
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MAND8 MAND10 MAND11 MAND12 MAND13 MAND14 MAND15
Wear Hair Net Wear Face Mask Wear Hand Wear Respiralory  Wear High Visibility ~ Pedestrian Route  Wear Safety Hamess
Protection Protection Clothing
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MAND16 MAND17 MAND18 MAND19 MAND20 MAND21 MAND23
Wash Your Hands Check Guard Use Adjustable Keep Locked Sound Hom Lift Correctly Wear Anti-Static
Guard Footwear

MAND24 MAND25 MAND26 MAND27 MAND28 MAND29 MAND30

Wear Laboratory ~ Wear Life Jacket UselitlerBin  Switch OffAfter Use  Wear Seatbelt Use Ladder Use Stairs
Coat

MAND36 MANDA0 MAND41 MAND42 MAND43 MAND44 MANDAS
ConnectAnEarth  Wear Protective  Referto Instruction  Disconnect From Use Handrail Disconnect Before  Use Barrier Cream
Terminal To The Apron Manual/Booklet Mains Supply Carrying Out

Ground Maintenance/Repair

e
@

MAND46 MAND47
Use Footbridge  Wear Opaque Eye
Protection
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