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	COSHH ASSESSMENT
CONTROL OF SUBSTANCES HAZARDOUS TO HEALTH REGULATIONS 2002
	[image: ]

	ADBLUE

	Hazardous Contents:
	



	GENERAL RISKS & CONTROLS

	Classification (state the category of danger)

	[image: ]
	☐	Serious Health Hazard/Toxic
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	☒	Oxidising
	[image: ]
	☐	Gas Under Pressure
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	☐	Health Hazard/ Harmful/Irritant
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	☐	Flammable
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	☐	Acute Toxicity/ Carcinogen
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	☐	Corrosive
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	☐	Explosive
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	☒	Dangerous for the Environment

	Hazard Type

	☐	☐	☐	☐	☐	☒	☐	☐
	Gas
	Water
	Mist
	Fume
	Dust
	Liquid
	Solid
	Other

	Route of Exposure

	☒	☒	☒	☒	☐	

	Inhalation
	Skin
	Eyes
	Ingestion
	Other (state)
	

	

	Workplace Exposure Limits (WELs) please indicate n/a where not applicable
	
NONE IDENTIFIED.

	Storage & Handling
	Hazard Symptoms

	· Store in locked COSHH store until required.
· Store in cool well ventilated area, with container tightly closed.
· Keep away from fire and heat sources. Avoid strong oxidising agents.
· Do NOT remove labels, avoid subsoil penetration.
	· May cause slight eye irritation.
· May cause stomach pains, and diarrhoea.
· Fire causes formation of toxic fumes.
· Prolonged inhalation may cause dizziness, nausea, and headaches.
· Spilling paint may cause permanent colour change/damage to materials.
· May cause irritation to skin with repeated and prolonged exposure.

	Controls
	Remedial Actions

	· Avoid contact with eyes. Wear eye protection if splashing is likely.
· Do NOT eat, drink, smoke when using. Wash hands after use.
· Store/use away from fire and heat sources. Do NOT burn or incinerate empty or full containers.
· Use in well ventilated area. If necessary wear appropriate RPE.
· Ensure spill kit is available, and splash controls are implemented such as covering of surfaces with protective sheeting
· Wear impermeable gloves, and overalls if necessary.
	· - Stop spillage immediately if safe to do so.
· - Ensure adequate ventilation.
· - Do NOT allow release into drains, sewers, or water courses.
· - Absorb with absorbent material.
· - If spilt into water, contain using a boom, and remove by skimming and absorbent material.
· - Wash contaminated area thoroughly after spillage.

	Disposal

	Hazardous Waste?
 ☐
	Skip
☒
	Other ☒
· Dispose of using licensed waste disposal site in accordance with local authority.
· Recycle packaging where applicable.
· Do NOT burn or incinerate.

	Return to Depot 
☐
	Return to Supplier
☐
	

	FIRST AID
[image: ]
	FIRE FIGHTING
[image: ]


	· Remove person from source of exposure. Keep at rest. If discomfort continues seek medical attention.
· Remove contaminated cloths. Wash skin thoroughly with water. If irritation occurs, seek medical attention.
	· Remove any contact lenses and flush eyes with water, continue for 15 minutes. 
· Seek medical attention if irritation occurs.
· - Rinse mouth with water, do NOT induce vomiting, and seek medical attention if any discomfort occurs.
	WATER
☒
	FOAM
☒
	POWDER
☒
	CO2
☒
	CHEMICAL
☒

	· 
	· 
	PRECAUTIONS:
Use media best suited to surrounding materials. Fire causes formation of toxic fumes.


	SITE SPECIFIC CONTROLS (TO BE COMPLETED ON SITE)

	Work Activities Being Undertaken

	Filling plant on site 

	Exposure

	Number of Persons
	Frequency
	Duration
	Any specific training requirements?

	5 -10 
	Daily 
	8 hours 
	☒
	Personal Protective Equipment (PPE) Control Measures
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	☒	☐	☒	☒	☐	☐	☒	☐	☐
	Eye Protection
	Ear Protection
	Hard Hat
	Footwear
	Overalls
	Visor
	Gloves
	Face Mask
	Respirator

	
	
	
	
	
	
	
	
	

	Storage Requirements

	
LOCKED CAGE
	BUNDED CONTAINER
	PROTECTION
FROM WEATHER
	COSHH STORAGE ROOM
	
SEALED CONTAINER

	☐	☐	☐	☒	☐
	Waste Management

	SEGREGATED STORAGE
	SEALED CONTAINERS
	WASTE CARRIER DISPOSAL / RECYCLING LICENCE

	☐	☒	☐
	Risk Rating Following Control Measures

	LOW
	MEDIUM
	HIGH

	☒	☐	☐


	Site Specific RA Prepared by:
	Si King 
	Position:
	Contracts Director 

	
	
	Review Date:
	27/09/2023
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Mandatory Symbols
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MAND1 MAND2 MAND3 MAND4 MANDS MANDG MAND?
General Mandatory ~ Wear Hearing  Wear Eye Protection WearHead ~ Wear Foot Protection  Wear Protective  Wear Face Shield
Action Protection Protection Clothing
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MAND8 MAND10 MAND11 MAND12 MAND13 MAND14 MAND15
Wear Hair Net Wear Face Mask Wear Hand Wear Respiralory  Wear High Visibility ~ Pedestrian Route  Wear Safety Hamess
Protection Protection Clothing

N
©
A
L
@

O

MAND16 MAND17 MAND18 MAND19 MAND20 MAND21 MAND23
Wash Your Hands Check Guard Use Adjustable Keep Locked Sound Hom Lift Correctly Wear Anti-Static
Guard Footwear

MAND24 MAND25 MAND26 MAND27 MAND28 MAND29 MAND30

Wear Laboratory ~ Wear Life Jacket UselitlerBin  Switch OffAfter Use  Wear Seatbelt Use Ladder Use Stairs
Coat

MAND36 MANDA0 MAND41 MAND42 MAND43 MAND44 MANDAS
ConnectAnEarth  Wear Protective  Referto Instruction  Disconnect From Use Handrail Disconnect Before  Use Barrier Cream
Terminal To The Apron Manual/Booklet Mains Supply Carrying Out

Ground Maintenance/Repair

e
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MAND46 MAND47
Use Footbridge  Wear Opaque Eye
Protection
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