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	COSHH ASSESSMENT
CONTROL OF SUBSTANCES HAZARDOUS TO HEALTH REGULATIONS 2002
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	GREASE LUBRICANT

	Hazardous Contents:
	Zinc Dialkyldithiophosphate.



	GENERAL RISKS & CONTROLS

	Classification (state the category of danger)

	[image: ]
	☐	Serious Health Hazard/Toxic
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	☐	Oxidising
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	☐	Gas Under Pressure
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	☒	Health Hazard/ Harmful/Irritant
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	☐	Flammable
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	☐	Acute Toxicity/ Carcinogen
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	☐	Corrosive
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	☐	Explosive
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	☒	Dangerous for the Environment

	Hazard Type

	☐	☐	☐	☐	☐	☒	☐	☐
	Gas
	Water
	Mist
	Fume
	Dust
	Liquid
	Solid
	Other

	Route of Exposure

	☒	☒	☒	☐	☐	

	Inhalation
	Skin
	Eyes
	Ingestion
	Other (state)
	

	

	Workplace Exposure Limits (WELs) please indicate n/a where not applicable
	5mg/m3
TWA

	Storage & Handling
	Hazard Symptoms

	· Store in cool, well ventilated area, in original container on an impermeable floor and away from acids.
· Avoid sources of ignition and heat sources, and ingress of water.
· Do NOT remove labels. 
· Ensure container is protected from impact.
· Avoid strong oxidising agents, and strong acids.	
· Ensure container does not have residual grease on outside of container when lifting or handling.
	· In combustion emits toxic fumes.
· Release into the environment causes damage to aquatic organisms.
· Container may be slippery due to residual grease left on the container.
· Creates slippery surface.
· Ingesting substance can cause diarrhoea and stomach pains.
· Extended exposure to skin can cause irritation and dermatitis.
· Contact with the eyes will cause irritation.

	Controls
	Remedial Actions

	· Avoid leaving the substance close to sources of extreme temperature, oxidising agents, and strong acids.
· Store on impermeable ground. Use bund to ensure leaks to not contaminate the ground.
· Ensure container is adequately free from grease before lifting/handling. Use gloves with suitable grip, and mechanical aids were necessary.
· Clean up procedure if spilt: Absorb into dry earth or sand and dispose of waste accordingly.
· Do NOT eat, drink, smoke, when using. Maintain high level of hygiene.
· Wear impermeable protective gloves when handling.
· Wear protective eye wear.
	· Stop the spill if safe to do so.
· Prevent entry into drains, sewers, and watercourses.
· Soak up with absorbent material.
· If spilt into water, contain by a boom, then collect by skimming or absorption.
· Clean the contaminated area, surface will be slippery.

	Disposal

	Hazardous Waste?
 ☐
	Skip
☒
	Other ☒
· Place used/contaminated materials in suitable containers.
· Do NOT burn or incinerate empty or full containers.
· Dispose of controlled waste using licenced waste disposal company.

	Return to Depot 
☐
	Return to Supplier
☐
	

	· FIRST AID
· [image: ]
	FIRE FIGHTING
[image: ]


	· No applicable. May exert toxic fumes when exposed to acids and combustion. In the event seek medical attention
· Remove contaminated cloths and wash with warm soap water immediately.
· Seek medical attention if irritation continues.
	· Remove contact lenses and flush eye immediately with water. Seek medical attention if discomfort continues.
· Wash mouth out with water. Do not induce vomiting. Seek medical attention if discomfort continues.
	WATER
☒
	FOAM
☒
	POWDER
☒
	CO2
☒
	CHEMICAL
☒

	· 
	· 
	PRECAUTIONS:
Combustion emits toxic fumes. Use media best suited for surroundings.


	SITE SPECIFIC CONTROLS (TO BE COMPLETED ON SITE)

	Work Activities Being Undertaken

	Fuelling of Plant & Equipment on site

	Exposure

	Number of Persons
	Frequency
	Duration
	Any specific training requirements?

	5-10
	Daily
	30 mins
	☐
	Personal Protective Equipment (PPE) Control Measures

	[image: ]
	[image: ]
	[image: ]
	[image: ]
	[image: ]
	[image: ]
	[image: ]
	[image: ]
	[image: ]

	☐	☐	☐	☐	☐	☐	☐	☐	☐
	Eye Protection
	Ear Protection
	Hard Hat
	Footwear
	Overalls
	Visor
	Gloves
	Face Mask
	Respirator

	
	
	
	
	
	
	
	
	

	Storage Requirements

	
LOCKED CAGE
	BUNDED CONTAINER
	PROTECTION
FROM WEATHER
	COSHH STORAGE ROOM
	
SEALED CONTAINER

	☐	☐	☐	☐	☐
	Waste Management

	SEGREGATED STORAGE
	SEALED CONTAINERS
	WASTE CARRIER DISPOSAL / RECYCLING LICENCE

	☐	☒	☐
	Risk Rating Following Control Measures

	LOW
	MEDIUM
	HIGH

	☐	☐	☐


	Site Specific RA Prepared by:
	Si King 
	Position:
	Contracts Director 

	
	
	Review Date:
	27/09/2023
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Mandatory Symbols
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MAND1 MAND2 MAND3 MAND4 MANDS MANDG MAND?
General Mandatory ~ Wear Hearing  Wear Eye Protection WearHead ~ Wear Foot Protection  Wear Protective  Wear Face Shield
Action Protection Protection Clothing
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MAND8 MAND10 MAND11 MAND12 MAND13 MAND14 MAND15
Wear Hair Net Wear Face Mask Wear Hand Wear Respiralory  Wear High Visibility ~ Pedestrian Route  Wear Safety Hamess
Protection Protection Clothing
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MAND16 MAND17 MAND18 MAND19 MAND20 MAND21 MAND23
Wash Your Hands Check Guard Use Adjustable Keep Locked Sound Hom Lift Correctly Wear Anti-Static
Guard Footwear

MAND24 MAND25 MAND26 MAND27 MAND28 MAND29 MAND30

Wear Laboratory ~ Wear Life Jacket UselitlerBin  Switch OffAfter Use  Wear Seatbelt Use Ladder Use Stairs
Coat

MAND36 MANDA0 MAND41 MAND42 MAND43 MAND44 MANDAS
ConnectAnEarth  Wear Protective  Referto Instruction  Disconnect From Use Handrail Disconnect Before  Use Barrier Cream
Terminal To The Apron Manual/Booklet Mains Supply Carrying Out

Ground Maintenance/Repair

e
@

MAND46 MAND47
Use Footbridge  Wear Opaque Eye
Protection
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