	CA019
	COSHH ASSESSMENT
CONTROL OF SUBSTANCES HAZARDOUS TO HEALTH REGULATIONS 2002
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	Hydraulic Oil

	Hazardous Contents:
	C15-C19 Alkanes. Zn Dialkyldithiophoshate. Alkylphenol. Synthetic. Neutral.
Calcium Petroleum sulphonate.




	GENERAL RISKS & CONTROLS

	Classification (state the category of danger)
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	☐	Serious Health Hazard/Toxic
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	☐	Oxidising
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	☐	Gas Under Pressure
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	☒	Health Hazard/ Harmful/Irritant
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	☐	Flammable
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	☐	Acute Toxicity/ Carcinogen
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	☐	Corrosive
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	☐	Explosive
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	☒	Dangerous for the Environment

	Hazard Type

	☐	☐	☐	☐	☐	☒	☐	☐
	Gas
	Water
	Mist
	Fume
	Dust
	Liquid
	Solid
	Other

	Route of Exposure

	☒	☒	☒	☒	☐	

	Inhalation
	Skin
	Eyes
	Ingestion
	Other (state)
	

	

	Workplace Exposure Limits (WELs) please indicate n/a where not applicable
	
10mg/15mins

	Storage & Handling
	Hazard Symptoms

	· Keep substance in original container tightly closed. 
· Avoid sources of heat and ignition, and ingress of water. 
· A bund area is required (110% percent capacity of container.) 
· Keep on impermeable ground. 
· Do NOT remove labels. 
· Protect against impact and puncture.
	· Substance may cause slight skin irritation.
· May cause slight eye irritation. 
· Ingestion may cause gastrointestinal irritation, nausea, vomiting and diarrhoea. 
· Harmful to aquatic organisms. 
· Barrels are heavy even when empty.
· Inheritably combustible.

	Controls
	Remedial Actions

	· Wear impermeable gloves, and overalls where necessary.
· Avoid contact with the eyes. Use eye protection.
· Do NOT siphon by mouth. Do NOT eat, drink smoke when using, and wash hands after use.
· Store on bund, on impermeable grounds. Keep spill kit close by.
· Use mechanical aids, and manual handling techniques when handling. Do NOT drag, roll, or push drums.
· Keep away from open flames, heat, hot surfaces, and other sources of ignition.
	· Stop the spill if safe to do so.
· Prevent entry into drains, sewers, and watercourses.
· Soak up with absorbent material.
· If spilt into water, contain by a boom, then collect by skimming or
· absorption.
· Clean the contaminated area, surface will be slippery.
· Notify Environmental agency if spill contaminates water.

	Disposal

	Hazardous Waste?
 ☐
	Skip
☒
	·  Place used/contaminated materials in suitable containers. - Dispose of controlled waste in accordance with Duty of Care Regs (Environmental Protection Act 1990-Section34) Using a licenced waste disposal company. - Do NOT burn or incinerate drums.                      Other ☐

	Return to Depot 
☐
	Return to Supplier
☐
	

	FIRST AID
[image: ]
	FIRE FIGHTING
[image: ]


	Remove to fresh air. If effects persist, seek medical attention.
Wash thoroughly with warm soap water. Seek medical attention if irritation occurs.
	 Remove contact lenses, and flush with water. If irritation continues get medical attention.

 Rinse mouth with water. Do NOT induce vomiting, unless instructed by a medical professional.
	WATER
☒
	FOAM
☒
	POWDER
☒
	CO2
☐
	CHEMICAL
☐

	· 
	· 
	PRECAUTIONS:



	SITE SPECIFIC CONTROLS (TO BE COMPLETED ON SITE)

	Work Activities Being Undertaken

	Fuelling of Plant & Equipment on site

	Exposure

	Number of Persons
	Frequency
	Duration
	Any specific training requirements?

	5-10
	Daily
	30 mins
	☐
	Personal Protective Equipment (PPE) Control Measures
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	☐	☐	☐	☐	☐	☐	☐	☐	☐
	Eye Protection
	Ear Protection
	Hard Hat
	Footwear
	Overalls
	Visor
	Gloves
	Face Mask
	Respirator

	
	
	
	
	
	
	
	
	

	Storage Requirements

	
LOCKED CAGE
	BUNDED CONTAINER
	PROTECTION
FROM WEATHER
	COSHH STORAGE ROOM
	
SEALED CONTAINER

	☐	☐	☐	☐	☐
	Waste Management

	SEGREGATED STORAGE
	SEALED CONTAINERS
	WASTE CARRIER DISPOSAL / RECYCLING LICENCE

	☐	☒	☐
	Risk Rating Following Control Measures

	LOW
	MEDIUM
	HIGH

	☐	☒	☐


	Site Specific RA Prepared by:
	Si King  
	Position:
	Contracts Director  

	
	
	Review Date:
	28/09/2023
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Mandatory Symbols
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MAND1 MAND2 MAND3 MAND4 MANDS MANDG MAND?
General Mandatory ~ Wear Hearing  Wear Eye Protection WearHead ~ Wear Foot Protection  Wear Protective  Wear Face Shield
Action Protection Protection Clothing
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MAND8 MAND10 MAND11 MAND12 MAND13 MAND14 MAND15
Wear Hair Net Wear Face Mask Wear Hand Wear Respiralory  Wear High Visibility ~ Pedestrian Route  Wear Safety Hamess
Protection Protection Clothing
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MAND16 MAND17 MAND18 MAND19 MAND20 MAND21 MAND23
Wash Your Hands Check Guard Use Adjustable Keep Locked Sound Hom Lift Correctly Wear Anti-Static
Guard Footwear

MAND24 MAND25 MAND26 MAND27 MAND28 MAND29 MAND30

Wear Laboratory ~ Wear Life Jacket UselitlerBin  Switch OffAfter Use  Wear Seatbelt Use Ladder Use Stairs
Coat

MAND36 MANDA0 MAND41 MAND42 MAND43 MAND44 MANDAS
ConnectAnEarth  Wear Protective  Referto Instruction  Disconnect From Use Handrail Disconnect Before  Use Barrier Cream
Terminal To The Apron Manual/Booklet Mains Supply Carrying Out

Ground Maintenance/Repair

e
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MAND46 MAND47
Use Footbridge  Wear Opaque Eye
Protection
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