	CA017
	COSHH ASSESSMENT
CONTROL OF SUBSTANCES HAZARDOUS TO HEALTH REGULATIONS 2002
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	Plasterboard

	Hazardous Contents:
	Silica. Quartz.



	GENERAL RISKS & CONTROLS

	Classification (state the category of danger)
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	☐	Serious Health Hazard/Toxic
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	☐	Oxidising
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	☐	Gas Under Pressure
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	☐	Health Hazard/ Harmful/Irritant
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	☐	Flammable
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	☐	Acute Toxicity/ Carcinogen
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	☐	Corrosive
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	☐	Explosive
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	☒	Dangerous for the Environment

	Hazard Type

	☐	☐	☐	☐	☒	☐	☒	☐
	Gas
	Water
	Mist
	Fume
	Dust
	Liquid
	Solid
	Other

	Route of Exposure

	☒	☒	☒	☒	☐	

	Inhalation
	Skin
	Eyes
	Ingestion
	Other (state)
	

	

	Workplace Exposure Limits (WELs) please indicate n/a where not applicable
	10mg /8 hour

	Storage & Handling
	Hazard Symptoms

	· Store on stable pallets on even ground
· Ensure plaster boards do not fall, or can be blown over.  Protect against the weather, prevent the ingress of   moisture.
· Ensure substance is laid flat.
· Use mechanical aids when handling, substance may come in awkward sizes.
	· May irritate the respiratory system, skin and eyes. Plasters may produce an alkaline solution on contact with body moisture or when mixed with water. 
· Plasterboard can NOT take the weight of any person. 
· Avoid mechanical cutting equipment. Cutting material causes dust to eject into the atmosphere.
· Heavy in large quantities, and awkward to handle.

	Controls
	Remedial Actions

	· Wear overalls to prevent contact with skin. Ensure good ventilation of working area.
· Wear protective gloves to avoid prolonged or repeated contact. Exclude unauthorised persons from the area.
· General training in the safe use, handling, disposal and storage, instruction in the use of control measures.
· Remove as a whole wherever possible. Wet down prior and during removal to reduce levels of dust. Hand cut were possible. If dust cannot be sufficiently controlled when cutting or breaking use appropriate RPE and isolate the working area.
· When handling large quantities, ensure mechanical aids are implemented, and manual handling techniques are used.
	· Stop the process creating the release.
· Dampen down the area, and allow for ventilation.
· Dry sweep/vacuum large amounts using adequate RPE.
· Wet mop and rinse contaminated area for residual dust.
· Conduct monitoring to ensure dust is back to an acceptable level

	Disposal

	Hazardous Waste?
 ☐
	Skip
☒
	Other ☒
· Fully recyclable classified as EWC 17 08 02. 
· Store waste separate from all other waste.

	Return to Depot 
☐
	Return to Supplier
☐
	

	FIRST AID
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	FIRE FIGHTING
[image: ]


	· Remove casualty to fresh air, and keep warm and at rest. If irritation occurs, seek medical advice.

·  Wash skin with plenty of warm soap water. Apply moisturising lotion. If irritation occurs, seek medical advice.
	· Remove any contact lenses, flush eyes with water. Repeat for 15mins. Seek medical attention if irritation occurs.

· Do NOT induce vomiting. Rinse mouth with clean water. Seek medical attention if irritation occurs.
	WATER
☒
	FOAM
☒
	POWDER
☒
	CO2
☒
	CHEMICAL
☒

	· 
	· 
	PRECAUTIONS: NOT a fire hazard, packaging may burn.



	SITE SPECIFIC CONTROLS (TO BE COMPLETED ON SITE)

	Work Activities Being Undertaken

	

	Exposure

	Number of Persons
	Frequency
	Duration
	Any specific training requirements?

	5 -10 
	Daily 
	8 hours 
	☐
	Personal Protective Equipment (PPE) Control Measures
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	☒	☐	☒	☒	☐	☐	☒	☒	☐
	Eye Protection
	Ear Protection
	Hard Hat
	Footwear
	Overalls
	Visor
	Gloves
	Face Mask
	Respirator

	
	
	
	
	
	
	
	
	

	Storage Requirements

	
LOCKED CAGE
	BUNDED CONTAINER
	PROTECTION
FROM WEATHER
	COSHH STORAGE ROOM
	
SEALED CONTAINER

	☐	☐	☒	☐	☐
	Waste Management

	SEGREGATED STORAGE
	SEALED CONTAINERS
	WASTE CARRIER DISPOSAL / RECYCLING LICENCE

	☐	☒	☒
	Risk Rating Following Control Measures

	LOW
	MEDIUM
	HIGH

	☐	☐	☐


	Site Specific RA Prepared by:
	Si King 
	Position:
	Contracts Director 

	
	
	Review Date:
	28/09/2023
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Mandatory Symbols
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MAND1 MAND2 MAND3 MAND4 MANDS MANDG MAND?
General Mandatory ~ Wear Hearing  Wear Eye Protection WearHead ~ Wear Foot Protection  Wear Protective  Wear Face Shield
Action Protection Protection Clothing
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MAND8 MAND10 MAND11 MAND12 MAND13 MAND14 MAND15
Wear Hair Net Wear Face Mask Wear Hand Wear Respiralory  Wear High Visibility ~ Pedestrian Route  Wear Safety Hamess
Protection Protection Clothing
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MAND16 MAND17 MAND18 MAND19 MAND20 MAND21 MAND23
Wash Your Hands Check Guard Use Adjustable Keep Locked Sound Hom Lift Correctly Wear Anti-Static
Guard Footwear

MAND24 MAND25 MAND26 MAND27 MAND28 MAND29 MAND30

Wear Laboratory ~ Wear Life Jacket UselitlerBin  Switch OffAfter Use  Wear Seatbelt Use Ladder Use Stairs
Coat

MAND36 MANDA0 MAND41 MAND42 MAND43 MAND44 MANDAS
ConnectAnEarth  Wear Protective  Referto Instruction  Disconnect From Use Handrail Disconnect Before  Use Barrier Cream
Terminal To The Apron Manual/Booklet Mains Supply Carrying Out

Ground Maintenance/Repair

e
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MAND46 MAND47
Use Footbridge  Wear Opaque Eye
Protection
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