

	CA013
	COSHH ASSESSMENT
CONTROL OF SUBSTANCES HAZARDOUS TO HEALTH REGULATIONS 2002
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	Bleach 

	Hazardous Contents:
	Sodium Hypochlorite. Alcohol Ethoxylate.



	GENERAL RISKS & CONTROLS

	Classification (state the category of danger)
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	☐	Serious Health Hazard/Toxic
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	☐	Oxidising
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	☐	Gas Under Pressure
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	☒	Health Hazard/ Harmful/Irritant
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	☐	Flammable
	[image: ]
	☐	Acute Toxicity/ Carcinogen
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	☒	Corrosive
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	☐	Explosive
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	☒	Dangerous for the Environment

	Hazard Type

	☐	☐	☐	☐	☐	☒	☐	☐
	Gas
	Water
	Mist
	Fume
	Dust
	Liquid
	Solid
	Other

	Route of Exposure

	☒	☒	☒	☒	☐	

	Inhalation
	Skin
	Eyes
	Ingestion
	Other (state)
	

	

	Workplace Exposure Limits (WELs) please indicate n/a where not applicable
	
2mg/15mins

	Storage & Handling
	Hazard Symptoms

	· Keep in original. 
· Keep container tightly closed. 
· Keep in locked COSHH store in a cool, well ventilated area away from food and water. 
· Store separate from acids. 
· Avoid possible impact and puncture. 
· Store away from sources of heat and ignition.
	· Will severely irritate eyes. 
· Contact with the skin may cause burns. 
· Respiration may cause irritation. 
· May cause burning on ingestion. 
· Fire/burning can create toxic gasses. 
· Surfaces may become slippery.

	Controls
	Remedial Actions

	· Wear appropriate eye protection, avoid contact with the eyes.
· Wear impermeable gloves, and overalls were necessary.
· Ensure usage is in a well ventilated area. Wear RPE if required.
· Do NOT eat, drink or smoke when using. Wash hands thoroughly after use.
· Use/store away from potential sources of heat and ignition. Only store amount required. Do NOT over stock.
· Do NOT decant into other containers. 
· General information and training on usage, storing, handling, controls, and disposal before using product.
	· Stop the spillage if safe to do so.
· Prevent entry into drains, sewers, and watercourses.
· Use absorbent material to absorb the spill.
· Small spillages can be flushed away with water.
· Clean area with water thoroughly. Area may become slippery

	Disposal

	Hazardous Waste?
 ☐
	Skip
☒
	· Do not pore into drains or water courses.
· Dispose in accordance with local authority requirements. Recycle if practicable. 
· Do NOT burn or incinerate container.

	Return to Depot 
☐
	Return to Supplier
☐
	

	FIRST AID
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	FIRE FIGHTING
[image: ]


	· Remove victim immediately from souse of exposure. Seek medical advice if irritation continues.
· Remove contaminated cloths, and wash skin thoroughly with warm soap water. - Use suitable lotion to moisturise skin. Get medical advice with irritation continues.
	· Remove contact lenses. Flush eyes with water, get medical attention if irritation persists.

· Rinse mouth thoroughly, Drink plenty of water. Seek medical attention immediately if irritation occurs.
	WATER
☒
	FOAM
☒
	POWDER
☒
	CO2
☐
	CHEMICAL
☐

	· 
	· 
	PRECAUTIONS: NOT flammable. Fire causes formation of toxic gasses. Prevent water runoff into water sources.



	SITE SPECIFIC CONTROLS (TO BE COMPLETED ON SITE)

	Work Activities Being Undertaken

	

	Exposure

	Number of Persons
	Frequency
	Duration
	Any specific training requirements?

	5 -10 
	Daily 
	8 Hours 
	☐
	Personal Protective Equipment (PPE) Control Measures
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	☒	☐	☒	☒	☐	☐	☒	☒	☐
	Eye Protection
	Ear Protection
	Hard Hat
	Footwear
	Overalls
	Visor
	Gloves
	Face Mask
	Respirator

	
	
	
	
	
	
	
	
	

	Storage Requirements

	
LOCKED CAGE
	BUNDED CONTAINER
	PROTECTION
FROM WEATHER
	COSHH STORAGE ROOM
	
SEALED CONTAINER

	☐	☐	☐	☒	☐
	Waste Management

	SEGREGATED STORAGE
	SEALED CONTAINERS
	WASTE CARRIER DISPOSAL / RECYCLING LICENCE

	☐	☒	☐
	Risk Rating Following Control Measures

	LOW
	MEDIUM
	HIGH

	☐	☒	☐


	Site Specific RA Prepared by:
	Si King 
	Position:
	Contracts Director  

	
	
	Review Date:
	28/09/2023
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Mandatory Symbols
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MAND1 MAND2 MAND3 MAND4 MANDS MANDG MAND?
General Mandatory ~ Wear Hearing  Wear Eye Protection WearHead ~ Wear Foot Protection  Wear Protective  Wear Face Shield
Action Protection Protection Clothing
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MAND8 MAND10 MAND11 MAND12 MAND13 MAND14 MAND15
Wear Hair Net Wear Face Mask Wear Hand Wear Respiralory  Wear High Visibility ~ Pedestrian Route  Wear Safety Hamess
Protection Protection Clothing
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MAND16 MAND17 MAND18 MAND19 MAND20 MAND21 MAND23
Wash Your Hands Check Guard Use Adjustable Keep Locked Sound Hom Lift Correctly Wear Anti-Static
Guard Footwear

MAND24 MAND25 MAND26 MAND27 MAND28 MAND29 MAND30

Wear Laboratory ~ Wear Life Jacket UselitlerBin  Switch OffAfter Use  Wear Seatbelt Use Ladder Use Stairs
Coat

MAND36 MANDA0 MAND41 MAND42 MAND43 MAND44 MANDAS
ConnectAnEarth  Wear Protective  Referto Instruction  Disconnect From Use Handrail Disconnect Before  Use Barrier Cream
Terminal To The Apron Manual/Booklet Mains Supply Carrying Out

Ground Maintenance/Repair

e
@

MAND46 MAND47
Use Footbridge  Wear Opaque Eye
Protection
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