	CA005
	COSHH ASSESSMENT
CONTROL OF SUBSTANCES HAZARDOUS TO HEALTH REGULATIONS 2002
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	UNLEADED PETROL

	Hazardous Contents:
	Benzene. Gasoline. Toluene. Tert-butyl Methyl ether.	



	GENERAL RISKS & CONTROLS

	Classification (state the category of danger)
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	☐	Serious Health Hazard/Toxic
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	☐	Oxidising
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	☐	Gas Under Pressure
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	☒	Health Hazard/ Harmful/Irritant
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	☒	Flammable
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	☐	Acute Toxicity/ Carcinogen
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	☐	Corrosive
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	☒	Explosive
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	☒	Dangerous for the Environment

	Hazard Type

	☐	☐	☐	☐	☐	☒	☐	☐
	Gas
	Water
	Mist
	Fume
	Dust
	Liquid
	Solid
	Other

	Route of Exposure

	☒	☒	☒	☒	☐	

	Inhalation
	Skin
	Eyes
	Ingestion
	Other (state)
	

	

	Workplace Exposure Limits (WELs) please indicate n/a where not applicable
	
574mg/150ppm
15 minutes

	Storage & Handling
	Hazard Symptoms

	· Store in segregated, and approved area stood upright. Empty containers stored separately.
· Keep bund 110% capacity of container, on impermeable grounds, in cool and well-ventilated area. 
· Keep minimal amount of substance on site, store and use amount as its needed.
· Do not remove warning labels. Keep tightly closed.
· Keep away from sources of ignition, no smoking. Store away from possible sources of impact.
· Establish designated storage and refuelling area.
· Keep spill kits, and firefighting equipment stored close by.
	· Extremely flammable.
· Toxic to aquatic organisms.
· Fumes are heavier then air and will collect at low levels. Fumes may travel on declining surfaces and contaminate remote areas.
· Exposure to high levels of the vapour can cause irritation to eyes and mucous membranes, drowsiness leading to loss of consciousness.
· Ingestion of small amounts may cause nausea, diarrhoea; larger amounts may cause irritation, drowsiness and vomiting.
· Prolonged or repeated exposure may lead to short-term irritation, defatting of the skin and dermatitis.
· Contact with the eyes is likely to cause short-term irritation with redness and stinging.

	Controls
	Remedial Actions

	· Keep bund and on impermeable grounds.
· Avoid storage and use close to excavation, drains, basements, and confined spaces where fumes may accumulate. General training on specific hazards associated with substance.
· Do NOT Use close to ignition sources.
· Do NOT siphon by mouth. Wash hands after use. Do NOT eat, drink, smoke when using.
· Wear impermeable gloves. Avoid contact with the skin. Wear protective overalls were necessary.
· Wear appropriate eye protection.
	· Eliminate all sources of ignition.
· Ensure spill is absorbed with inert material.
· Dispose of/replace contaminated clothing.
· Do NOT allow entry into the environment.
· Keep all contaminated materials safely stored until disposal.

	Disposal

	Hazardous Waste?
 ☒
	Skip
☒
	Other ☒
· Dispose via an authorised person/Licensed disposal contractor in accordance to local regulations.
· Empty containers may contains residual substances, never weld, solder, braze, grind or heat.

	Return to Depot 
☐
	Return to Supplier
☐
	

	FIRST AID
[image: ]
	FIRE FIGHTING
[image: ]


	· If exposure causes drowsiness, headache, blurred vision, or irritation of the eyes, nose or throat, remove immediately to fresh air, keep patient warm and at rest. If symptoms persist, obtain medical advice.
· Wash skin thoroughly with warm soap water and remove heavily contaminated clothing to be washed.
· Seek medical advice if skin becomes red, swollen, or painful.
	· In case of eye contact, rinse immediately with water. Get medical attention if irritation continues.
· If swallowed, do not induce vomiting. Never give anything by mouth to an unconscious person.
· Aspiration hazard if swallowed, can enter lungs and cause damage, seek medical attention.
	WATER
☒
	FOAM
☒
	POWDER
☒
	CO2
☒
	CHEMICAL
☐

	· 
	· 
	PRECAUTIONS:
Do NOT use solid water Jet, use mist spray. Avoid residual water run-off into drains.


	SITE SPECIFIC CONTROLS (TO BE COMPLETED ON SITE)

	Work Activities Being Undertaken

	Generators 

	Exposure

	Number of Persons
	Frequency
	Duration
	Any specific training requirements?

	5 -10 
	Daily 
	8 hours 
	☐
	Personal Protective Equipment (PPE) Control Measures
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	☒	☐	☒	☒	☐	☐	☒	☐	☐
	Eye Protection
	Ear Protection
	Hard Hat
	Footwear
	Overalls
	Visor
	Gloves
	Face Mask
	Respirator

	
	
	
	
	
	
	
	
	

	Storage Requirements

	
LOCKED CAGE
	BUNDED CONTAINER
	PROTECTION
FROM WEATHER
	COSHH STORAGE ROOM
	
SEALED CONTAINER

	☐	☒	☐	☐	☐
	Waste Management

	SEGREGATED STORAGE
	SEALED CONTAINERS
	WASTE CARRIER DISPOSAL / RECYCLING LICENCE

	☐	☒	☐
	Risk Rating Following Control Measures

	LOW
	MEDIUM
	HIGH

	☐	☒	☒


	Site Specific RA Prepared by:
	Si King 
	Position:
	Contracts Director  

	
	
	Review Date:
	28/09/2023
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Mandatory Symbols
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MAND1 MAND2 MAND3 MAND4 MANDS MANDG MAND?
General Mandatory ~ Wear Hearing  Wear Eye Protection WearHead ~ Wear Foot Protection  Wear Protective  Wear Face Shield
Action Protection Protection Clothing
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MAND8 MAND10 MAND11 MAND12 MAND13 MAND14 MAND15
Wear Hair Net Wear Face Mask Wear Hand Wear Respiralory  Wear High Visibility ~ Pedestrian Route  Wear Safety Hamess
Protection Protection Clothing
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MAND16 MAND17 MAND18 MAND19 MAND20 MAND21 MAND23
Wash Your Hands Check Guard Use Adjustable Keep Locked Sound Hom Lift Correctly Wear Anti-Static
Guard Footwear

MAND24 MAND25 MAND26 MAND27 MAND28 MAND29 MAND30

Wear Laboratory ~ Wear Life Jacket UselitlerBin  Switch OffAfter Use  Wear Seatbelt Use Ladder Use Stairs
Coat

MAND36 MANDA0 MAND41 MAND42 MAND43 MAND44 MANDAS
ConnectAnEarth  Wear Protective  Referto Instruction  Disconnect From Use Handrail Disconnect Before  Use Barrier Cream
Terminal To The Apron Manual/Booklet Mains Supply Carrying Out

Ground Maintenance/Repair

e
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MAND46 MAND47
Use Footbridge  Wear Opaque Eye
Protection
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