	CA004
	COSHH ASSESSMENT
CONTROL OF SUBSTANCES HAZARDOUS TO HEALTH REGULATIONS 2002
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	Multi Spray Adhesive 

	Hazardous Contents:
	Butane/Isobutane. Dichloromethane. Propane.



	GENERAL RISKS & CONTROLS

	Classification (state the category of danger)
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	☐	Serious Health Hazard/Toxic
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	☐	Oxidising
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	☐	Gas Under Pressure
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	☒	Health Hazard/ Harmful/Irritant
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	☒	Flammable
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	☐	Acute Toxicity/ Carcinogen
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	☐	Corrosive
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	☐	Explosive
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	☐	Dangerous for the Environment

	Hazard Type

	☐	☐	☐	☐	☐	☒	☐	☐
	Gas
	Water
	Mist
	Fume
	Dust
	Liquid
	Solid
	Other

	Route of Exposure

	☒	☒	☒	☒	☐	

	Inhalation
	Skin
	Eyes
	Ingestion
	Other (state)
	

	

	Workplace Exposure Limits (WELs) please indicate n/a where not applicable
	
750ppm/1060mg 15mins

	Storage & Handling
	Hazard Symptoms

	· Store in original packaging. 
· Keep away from heat and sources of ignition.  
· General training in the safe use, handling, disposal and storage. 
· Store in locked COSHH store out of direct sunlight. 
· Avoid potential impact and puncture.
	· Extremely flammable. 
· Container is under pressure.
· Harmful by inhalation and if swallowed.
· Will defat skin and prolonged contact may produce dermatitis.
· Irritant to eyes.
· Limited evidence of a carcinogenic (causing cancer) effect.

	Controls
	Remedial Actions

	· Use away from heat and ignition sources.
· Do not pierce/puncture or incinerate even when container is empty.
· Ensure good ventilation and avoid use in confined spaces. Do NOT eat, drink, smoke while using. Wash hands after use.
· Ensure impermeable gloves are worn, wear overalls were necessary.
· Wear appropriate eye protection.
· Avoid prolonged contact with the substance.
	· Stop the spill if safe to do so.
· Clear any spillages using any available spill kit with absorbent
· material.
· Eliminate all sources of ignition.
· Ensure adequate ventilation
Do not allow entry into environment.

	Disposal

	Hazardous Waste?
 ☒
	Skip
☐
	Other ☒



Ensure that container is empty and dispose of according local authority regulations. 
Do not pierce or incinerate even when container is empty. 
Separate waste container for aerosol cans.


	Return to Depot 
☐
	Return to Supplier
☐
	

	FIRST AID
[image: ]
	FIRE FIGHTING
[image: ]


	Move exposed person to fresh air. Seek medical attention is discomfort continues.

  Promptly wash contaminated skin with soap or mild detergent and water. - Remove clothing is soaked through ad wash as above.
	Remove clothing is soaked through ad wash as above.

- Immediately flush eyes with waste while lifting the eye lid. Continue procedure for 15 minutes before seeking medical attention.

 - Rinse mouth thoroughly. Do not induce vomiting. Seek medical attention if irritation persist.
	WATER
☐
	FOAM
☒
	POWDER
☒
	CO2
☒
	CHEMICAL
☐

	· 
	· 
	PRECAUTIONS:

May explode in fire, May flash back. Forms explosive atmosphere. Do NOT use water jet, only spray/mist.


	SITE SPECIFIC CONTROLS (TO BE COMPLETED ON SITE)

	Work Activities Being Undertaken

	

	Exposure

	Number of Persons
	Frequency
	Duration
	Any specific training requirements?

	5 -10 
	Daily 
	8 Hiuyrs 
	☐
	Personal Protective Equipment (PPE) Control Measures
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	☒	☐	☒	☒	☐	☐	☒	☐	☐
	Eye Protection
	Ear Protection
	Hard Hat
	Footwear
	Overalls
	Visor
	Gloves
	Face Mask
	Respirator

	
	
	
	
	
	
	
	
	

	Storage Requirements

	
LOCKED CAGE
	BUNDED CONTAINER
	PROTECTION
FROM WEATHER
	COSHH STORAGE ROOM
	
SEALED CONTAINER

	☐	☐	☐	☒	☐
	Waste Management

	SEGREGATED STORAGE
	SEALED CONTAINERS
	WASTE CARRIER DISPOSAL / RECYCLING LICENCE

	☐	☒	☐
	Risk Rating Following Control Measures

	LOW
	MEDIUM
	HIGH

	☒	☐	☐


	Site Specific RA Prepared by:
	Si King 
	Position:
	Contracts Director 

	
	
	Review Date:
	28/09/2023
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Mandatory Symbols
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MAND1 MAND2 MAND3 MAND4 MANDS MANDG MAND?
General Mandatory ~ Wear Hearing  Wear Eye Protection WearHead ~ Wear Foot Protection  Wear Protective  Wear Face Shield
Action Protection Protection Clothing
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MAND8 MAND10 MAND11 MAND12 MAND13 MAND14 MAND15
Wear Hair Net Wear Face Mask Wear Hand Wear Respiralory  Wear High Visibility ~ Pedestrian Route  Wear Safety Hamess
Protection Protection Clothing
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MAND16 MAND17 MAND18 MAND19 MAND20 MAND21 MAND23
Wash Your Hands Check Guard Use Adjustable Keep Locked Sound Hom Lift Correctly Wear Anti-Static
Guard Footwear

MAND24 MAND25 MAND26 MAND27 MAND28 MAND29 MAND30

Wear Laboratory ~ Wear Life Jacket UselitlerBin  Switch OffAfter Use  Wear Seatbelt Use Ladder Use Stairs
Coat

MAND36 MANDA0 MAND41 MAND42 MAND43 MAND44 MANDAS
ConnectAnEarth  Wear Protective  Referto Instruction  Disconnect From Use Handrail Disconnect Before  Use Barrier Cream
Terminal To The Apron Manual/Booklet Mains Supply Carrying Out

Ground Maintenance/Repair

e
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MAND46 MAND47
Use Footbridge  Wear Opaque Eye
Protection
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