	CA006
	COSHH ASSESSMENT
CONTROL OF SUBSTANCES HAZARDOUS TO HEALTH REGULATIONS 2002
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	Cement

	Hazardous Contents:
	Crystalline silica.



	GENERAL RISKS & CONTROLS

	Classification (state the category of danger)
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	☐	Serious Health Hazard/Toxic
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	☐	Oxidising
	[image: ]
	☐	Gas Under Pressure
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	☒	Health Hazard/ Harmful/Irritant
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	☐	Flammable
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	☐	Acute Toxicity/ Carcinogen

	[image: ]
	☒	Corrosive
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	☐	Explosive
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	☒	Dangerous for the Environment

	Hazard Type

	☐	☐	☐	☐	☒	☐	☐	☐
	Gas
	Water
	Mist
	Fume
	Dust
	Liquid
	Solid
	Other

	Route of Exposure

	☒	☒	☒	☒	☐	

	Inhalation
	Skin
	Eyes
	Ingestion
	Other (state)
	

	

	Workplace Exposure Limits (WELs) please indicate n/a where not applicable
	
10mg/ 8 hours

	Storage & Handling
	Hazard Symptoms

	· Keep shielded from weather, and humid environments.
· Store away from objects that may puncture the packaging. 
· Cautions should be taken when manual handling due to weight of packaged substance. Use of mechanical aids is advised when dealing with large quantities. 
· Store away from aluminium powder as when mixed with wet cement hydrogen is produced. 
· Keep bulk supplies in shrink wrapped packaging were possible to prevent residual dust being released.
	· Cement may have an irritating effect on moist skin due to
transpiration or humidity.
· Prolonged contact with wet cement may cause serious chemical burns, and can develop without pain being felt. 
· Eye contact with cement, wet or dry, may cause serious and potentially irreversible injuries. 
· Frequent inhalation of large quantities of cement dust over a longer period increases the risk of developing lung disease. 
· Nerve endings may be damaged prior to skin burning, hence burning may occur without pain being felt at the time. 

	Controls
	Remedial Actions

	· Wear impermeable protective clothing to ensure that cement or any cement/water mix does NOT come in contact with the skin.
· Ensure that wet concrete does NOT enter the boots and that people do NOT kneel on wet concrete. Wear impermeable gloves.
· Wherever there is a risk of cement powder or cement/water mixtures entering the eye, wear dust proof goggles. Do not eat, drink, or smoke when using. Wash hands thoroughly after use.
· Ensure good ventilation or ensure suitable RPE is worn.
· When laying concrete, impermeable gloves, boots, and trousers will be necessary. General awareness talks on delayed effects.
	· Do NOT wash cement down sewers, drains, watercourses.
· Recover the spillage in a dry state if possible.
· Use clean-up methods that do NOT cause airborne dispersion. Use wet mop/vacuum.
· Collect wet cement and place in container.
· Ensure all cement has hardened before disposal.

	Disposal

	Hazardous Waste?
 ☐
	Skip
☒
	Other ☒
 Do NOT use after use by date. 
 Do NOT flush into sewers, drains, watercourses. 
 Dispose or recycle according to local authority

	Return to Depot 
☐
	Return to Supplier
☐
	

	FIRST AID
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	FIRE FIGHTING
[image: ]


	Move person to fresh air. If discomfort persist, seek medical attention.

Remove any contaminated cloths. Wash off with plenty of water, seek medical attention if irritation continues.
	Do NOT rub eyes. Remove any contact lenses and flush with water. (Use isotonic water if able to.) - Seek medical attention if irritation continues.

 If ingested do NOT induce vomiting. Wash out mouth with plenty of water, seek medical advice if irritation persists.
	WATER
☒
	FOAM
☒
	POWDER
☒
	CO2
☒
	CHEMICAL
☒

	· 
	· 
	PRECAUTIONS

Use extinguishing method best suited for surrounding materials.


	SITE SPECIFIC CONTROLS (TO BE COMPLETED ON SITE)

	Work Activities Being Undertaken

	Exposure

	Number of Persons
	Frequency
	Duration
	Any specific training requirements?

	5 -10 
	Daily 
	8 Hours 
	☐
	Personal Protective Equipment (PPE) Control Measures
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	☒	☐	☒	☒	☐	☐	☒	☒	☐
	Eye Protection
	Ear Protection
	Hard Hat
	Footwear
	Overalls
	Visor
	Gloves
	Face Mask
	Respirator

	
	
	
	
	
	
	
	
	

	Storage Requirements

	
LOCKED CAGE
	BUNDED CONTAINER
	PROTECTION
FROM WEATHER
	COSHH STORAGE ROOM
	
SEALED CONTAINER

	☐	☐	☐	☐	☐
	Waste Management

	SEGREGATED STORAGE
	SEALED CONTAINERS
	WASTE CARRIER DISPOSAL / RECYCLING LICENCE

	☒	☒	☐
	Risk Rating Following Control Measures

	LOW
	MEDIUM
	HIGH

	☒	☐	☐


	Site Specific RA Prepared by:
	Si King 
	Position:
	Contracts Director 

	
	
	Review Date:
	28/09/2023
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Mandatory Symbols
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MAND1 MAND2 MAND3 MAND4 MANDS MANDG MAND?
General Mandatory ~ Wear Hearing  Wear Eye Protection WearHead ~ Wear Foot Protection  Wear Protective  Wear Face Shield
Action Protection Protection Clothing
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MAND8 MAND10 MAND11 MAND12 MAND13 MAND14 MAND15
Wear Hair Net Wear Face Mask Wear Hand Wear Respiralory  Wear High Visibility ~ Pedestrian Route  Wear Safety Hamess
Protection Protection Clothing
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MAND16 MAND17 MAND18 MAND19 MAND20 MAND21 MAND23
Wash Your Hands Check Guard Use Adjustable Keep Locked Sound Hom Lift Correctly Wear Anti-Static
Guard Footwear

MAND24 MAND25 MAND26 MAND27 MAND28 MAND29 MAND30

Wear Laboratory ~ Wear Life Jacket UselitlerBin  Switch OffAfter Use  Wear Seatbelt Use Ladder Use Stairs
Coat

MAND36 MANDA0 MAND41 MAND42 MAND43 MAND44 MANDAS
ConnectAnEarth  Wear Protective  Referto Instruction  Disconnect From Use Handrail Disconnect Before  Use Barrier Cream
Terminal To The Apron Manual/Booklet Mains Supply Carrying Out

Ground Maintenance/Repair

e
@

MAND46 MAND47
Use Footbridge  Wear Opaque Eye
Protection
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