

	CA012
	COSHH ASSESSMENT
CONTROL OF SUBSTANCES HAZARDOUS TO HEALTH REGULATIONS 2002
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	LINE MARKING SPRAY

	Hazardous Contents:
	Butoxyethanol. Methoxy. Propanol. Mixed Aromatic Hydrocarbons.



	GENERAL RISKS & CONTROLS

	Classification (state the category of danger)
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	☐	Serious Health Hazard/Toxic
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	☐	Oxidising
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	☐	Gas Under Pressure
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	☒	Health Hazard/ Harmful/Irritant
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	☒	Flammable
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	☒	Acute Toxicity/ Carcinogen
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	☐	Corrosive
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	☐	Explosive
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	☒	Dangerous for the Environment

	Hazard Type

	☐	☐	☐	☐	☐	☐	☐	☒
	Gas
	Water
	Mist
	Fume
	Dust
	Liquid
	Solid
	Other

	Route of Exposure

	☒	☒	☒	☒	☐	

	Inhalation
	Skin
	Eyes
	Ingestion
	Other (state)
	

	

	Workplace Exposure Limits (WELs) please indicate n/a where not applicable
	
25ppm
8 hour

	Storage & Handling
	Hazard Symptoms

	· Do not remove safety labels.
· Keep in locked COSHH store and well ventilated away from direct sunlight sources of heat and ignition.
· Store away from oxidising agents, and strong alkaline, and acidic materials.
· Protect against possible impact and puncture.
	· Extremely flammable. Risk of container explosion.
· May cause irritation if ingested.
· Repeated exposure to skin may cause skin dryness or cracking.
· Vapours may cause headache fatigue, dizziness and nausea.
· Irritant to eyes.
· Wet paint may make surfaces temporarily slippery.

	Controls
	Remedial Actions

	· Do NOT store or use close to heat or ignition sources. Do NOT smoke when using.
· Do NOT eat, drink, smoke when using, wash hands after use.
· Wear impermeable gloves, and overalls were necessary.
· Use in well ventilated area, or use appropriate RPE if required. Avoid use in confined spaces.
· Avoid contact with eyes, use eye protection.
· General training in the safe use, handling, disposal and storage, instruction in the use of control measures.
	· Eliminate all ignition sources.
· Stop the leak if safe to do so.
· Prevent entry into drains, sewers, and watercourses.
· Absorb spill using absorbent material.
· Store contaminated materials in sealed container.
· Wash contaminated area thoroughly with detergent.

	Disposal

	Hazardous Waste?
 ☒
	Skip
☐
	Other ☒
· Do NOT pore into drains/allow access into water courses.
· Dispose in accordance with the regulations made under the Control of Pollution Act.
· Do NOT burn or incinerate empty or full containers.

	Return to Depot 
☐
	Return to Supplier
☐
	

	FIRST AID
[image: ]
	FIRE FIGHTING
[image: ]


	·  Remove to fresh air, and keep warm and at rest. If breathing is irregular, or stopped, seek medical attention, or administer artificial respiration from a trained person.
· Remove contaminated clothing, and wash skin with warm soap water.
	· Remove contact lenses and rinse eyes immediately. Get medical attention if irritation persists.
· If swallowed, seek medical advice immediately and show container label. Do not induce vomiting.
	WATER
☒
	FOAM
☒
	POWDER
☒
	CO2
☒
	CHEMICAL
☐

	· 
	· 
	PRECAUTIONS:
Do NOT use solid water Jet, use mist spray. Avoid residual water run-off into drains.


	SITE SPECIFIC CONTROLS (TO BE COMPLETED ON SITE)

	Work Activities Being Undertaken

	

	Exposure

	Number of Persons
	Frequency
	Duration
	Any specific training requirements?

	5 -10
	Daily 
	8 Hours 
	☐
	Personal Protective Equipment (PPE) Control Measures
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	☒	☐	☒	☒	☐	☐	☒	☐	☐
	Eye Protection
	Ear Protection
	Hard Hat
	Footwear
	Overalls
	Visor
	Gloves
	Face Mask
	Respirator

	
	
	
	
	
	
	
	
	

	Storage Requirements

	
LOCKED CAGE
	BUNDED CONTAINER
	PROTECTION
FROM WEATHER
	COSHH STORAGE ROOM
	
SEALED CONTAINER

	☐	☐	☐	☒	☐
	Waste Management

	SEGREGATED STORAGE
	SEALED CONTAINERS
	WASTE CARRIER DISPOSAL / RECYCLING LICENCE

	☐	☒	☐
	Risk Rating Following Control Measures

	LOW
	MEDIUM
	HIGH

	☒	☒	☐


	Site Specific RA Prepared by:
	Si King 
	Position:
	Contracts Director 

	
	
	Review Date:
	27/09/2023
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Mandatory Symbols
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MAND1 MAND2 MAND3 MAND4 MANDS MANDG MAND?
General Mandatory ~ Wear Hearing  Wear Eye Protection WearHead ~ Wear Foot Protection  Wear Protective  Wear Face Shield
Action Protection Protection Clothing
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MAND8 MAND10 MAND11 MAND12 MAND13 MAND14 MAND15
Wear Hair Net Wear Face Mask Wear Hand Wear Respiralory  Wear High Visibility ~ Pedestrian Route  Wear Safety Hamess
Protection Protection Clothing
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MAND16 MAND17 MAND18 MAND19 MAND20 MAND21 MAND23
Wash Your Hands Check Guard Use Adjustable Keep Locked Sound Hom Lift Correctly Wear Anti-Static
Guard Footwear

MAND24 MAND25 MAND26 MAND27 MAND28 MAND29 MAND30

Wear Laboratory ~ Wear Life Jacket UselitlerBin  Switch OffAfter Use  Wear Seatbelt Use Ladder Use Stairs
Coat

MAND36 MANDA0 MAND41 MAND42 MAND43 MAND44 MANDAS
ConnectAnEarth  Wear Protective  Referto Instruction  Disconnect From Use Handrail Disconnect Before  Use Barrier Cream
Terminal To The Apron Manual/Booklet Mains Supply Carrying Out

Ground Maintenance/Repair

e
@

MAND46 MAND47
Use Footbridge  Wear Opaque Eye
Protection
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