Supporting measures
1. The floor level of the extensions will match the current floor level of the existing property and WILL NOT be any lower – see proposed elevations submitted.
2. The floor & walls will be constructed using the preferred construction methods outlined in the ‘Improving the flood performance of new buildings’
3. All electrical sockets will be set to a minimum of 450mm above finished floor level.
