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                                                                                                                                       December 2023

Cover system validation report overview document, 31A North Street, Emsworth, PO10 7DA

  
Sirs

Parchow Groundworks have been advised that there is some confusion that may have been inadvertently caused by the report that we’d previously issued.
   The purpose of this overview document is to explain the installation of the cover system in terms sequential process, and where appropriate, explain any deviation from the cover system noted with in the GCC RMS, albeit the change being one of an enhanced performance.
To aid understanding, the overview will deal with the bullet points noted by the HBC Environmental Control officer and then proceed to describe the works process to better understand the installation of the cover system and to enable all stakeholders to have adequate comfort in its efficacy and suitability for purpose.


Garden areas

The total garden areas given are accurate and indicate all areas that are subject to the specification shown in 4.3.2 of the GCC report indicating this. This area is 190.53m2. This covers the areas within the gardens inclusive of paths and patio’s etc

Conveyance proof

Page 8 of the previously submitted report may not have made clearly enough that there were in additional to the 2 TJ Transport Ltd topsoil loads an additional 3 delivered by Emmerson Transport Ltd.
  However, in addition to this there were a further 2400l’s of topsoil delivered from a merchant  and  a bulk delivery from Eurogreen Transport ltd from the same as the TJ & Emmerson deliveries that were not included. 
  Apologies, these are now appended to the overview document.


The 600mm cover system required 114.32m3 of topsoil volume and the deliveries noted, which equates to 6.35 loads, provide the required volume to comply with the RMS cover system design.

Retained made soils on site.

All materials noted in the images are in areas that are hard landscaped and not subject to the requirements of the cover system, as noted at the foot of 4.2 in the GCC report.
    Image 1 in the report is a perfect example of where all material within these areas were removed and replaced with BS3882 topsoil to the full section depth of 600mm within the area that the report targets for RMS cover system.


Works sequence

In order to mitigate against possible cross contamination, the works were broadly segregated between the North & East blocks so as to make them manageable and enable material to be tracked accurately on site.
    The East block was blocks were undertaken first, commencing 5/6/23. The unit’s green space areas were plotted by our setting out engineer and an area set aside between the 2 blocks with a sacrificial membrane placed to contain the made material that was being excavated prior to export from site.
The design formation level was 600mm below FGL, with discussions having taken place between PWP and HBC over the replacement of the biotic layer and the subsoil, with the replacement of both with BS3882 topsoil. The reasons for the change were manyfold but primarily that commercially available quantities of BS8601:2013 are very limited locally and as such, while not attractive for cost, replacing with the accredited topsoil assured us of the source characteristics that the GCC report required.
   Additionally, the change from 3 materials in the strata make-up to 1 simplified the process and thereby made errors of depth and contaminated layers far less likely.
Once at the formation level the site operatives placed Terram H-Viz anti-dig membrane [data sheet appended] in the area, ensuring that this abutted the hard landscaped areas sufficiently to alert anyone excavating in the future to the possible risks.
Upon completion of this stage of the process the BS3882 Topsoil was placed [between 12/6/23-15/6/23] directly in the excavation rather than placement elsewhere onsite, again to limit any possibility of cross-contamination.

The North block works commenced 15/6/23 with the same process undertaken regards using the proposed hard landscaped area between the blocks to temporarily store the export material away from the excavation. Again, formation level was established at 600mm below FGL and the Terram ani-dig barrier placed prior to the BS3882 topsoil being placed directly into the excavation.



















Appendix




· Merchant invoices for bagged topsoil
· Terram data sheet
· Haulier conveyance information for topsoil that was previously noted sent








[image: A close-up of a receipt

Description automatically generated]




[image: A close-up of a document

Description automatically generated]
[image: A close-up of a paper

Description automatically generated]




[image: A screenshot of a receipt

Description automatically generated]

image3.png
@ Travis Perkins

Travis Perkins Trading Company Limited
VAT Registration Number : GB 408 5567 37
Cheques Payable to : Travis Perkins Trading Co Lid.

POBoXs2T

INVOICE 3030 BDY208

INVOICE/TAXDATE : 03102123
DELIVERY NOTE  : E35870
DELIVERY DATE  : 0310223

ORDERNO. 06021086
NORTHAVPTON , N6 72E ACCONTNO - : WTass?
' REGION o0t
Parchow Groundworks Ltd DELVERED TO: COLLECTED
Widley Farm New Down Lane
Purbrook
WATERLOOVILLE
Hampshire
POT 5SE
Page 10i1
TTEn QUANTITY PRICE VALUE VAT
=) DESCRIPTION OF GOODS = e 3 P
663469 [SUPRGROW TOPSOL BULK BAG 8001 20 5 %, g
EAcH] e
purhasing Card N 900183622 for uying oo
Branch
PETERSFIELD TP G000 AMOUNT !
TRAVIS PERKINS TRADING CO. LTD
9 BEDFORD ROAD VAT TOTAL =
PETERSFIELD
Pt INVOICE TOTAL 8.
01730262233

TERMS NET MONTHLY

Registered in England No. 733503. Registered Office : Lodge Way House, Lodge Way, Harlesione Road, Northampton, NS 7UG.

Health & Safety: Fo information on producs (e.g. COSHH) piease
it o tEdsperkins. co.uk. Cortact the H&S Dept, dusig ofico.
hours on (01604) 752424 i cata ot aalable:

Pay your account balance online at:

www.travisperkins.co.uk




image4.png
HI-VIS

T1000 GEOTEXTILE

TERRAM Hi Vis is a non-woven orange geotextile used for
separating contaminated/ uncontaminated soils.

TERRAN Hi Vis geottles heve  dul efec: s vvid calour warns ofptential dangr o thepoint ofanyfture excations and t ca s prevent
the upward movement of ontaminated sol partdes.

TERRAM i Vis geoteeils provid aneffective sobtian ta the problem of » Paved and ungaved roads
constructing a stabl granuler ayar over soft foundtion i, When « Railvays

ston s paced dirctly o  sotsubgrade the inpused lad often causes = Car ks and hardstandings
intermixing of two layers. This results in cantsminatin of the stone leyer * Dycleways and footpaths
and  resuling loss inbearing strength, sufecs rutting and dformeton » SubS instalstions

tthe subbase/ subyade terfce + Bresnreofs

« Enginesred toprovide ighstrngthandhigh ongatio s reak

Whether it's a granular drain or a geosynthetic akernative such a5 apen « Manufactured from high tenscity UV stabilised viegin polyoropylene
gencelarurits, TERRAM Vs geotetle ae el for prevening the frs o provide ong term dursilty i ll o types
ingres offes.

= Manufacturad using s randorlyarientated web o rovid competly
isuropic properies

« allent unifrmity with i pemeabity ad low pae sz for soil

PRODUC 6 TI000 Grangs Beotertie Hiration
ol With (m) 45m)
ol Length m) 100 (m)

today or visit our website: Ground Protection and Reinforcement

www.groundtrax.com | Telephone: 03456 800008 | Fax: 03456 800208
E-Mail: info@groundtrax.com | Website: www.groundtrax.com

E"NE E For more information, contact us. GROU"DTRax




image5.png
VAT Reg No: 205520452

INVOICE Page 1
PARCHOW GROUNDWORKS LTD Invoice No 176999
NEW DOWN LANE
WATERLOOVILLE In Date 16/08/2023
HAMPSHIRE
PO7 55E Order No 406/8/560/P
Account Ref 04PARCHO
Quantity Description Unit Price DiscAmt  NetAmt VAT % VAT
1.00 BS3882 TOPSOIL - 8 WHEEL LOAD 420.00 000 42000 2000  84.00
0.00 TICKET 76613 0.00
DeliverTo : Total Discount £ 0.00
15.08.23
Rowlands Castle Road Total Net Amount | £ 420.00
Horndean
PO8 0AJ Carriage Net £ 0.00

Total Tax Amount £ 84.00

Invoice Total £ 504.00





image1.png
PARCHOW s
GROUNDWORKS LTD




image2.png
@ Travis Perkins

Travis Perkins Trading Company Limited
VAT Registration Number : GB 408 5567 37
Cheques Payable to : Travis Perkins Trading Co Ltd.

INVOICE 0568 ATY543

INVOICE/TAX DATE : 08107122
DELVERY NOTE - F21700
DELVERY DATE - 0807122

POBOXE27 ORDERNO. w6
NORTHAMPTON . NNS 72E ACCOUNTNO : WTass7
REGION 3
Parchow Groundworks Ltd DELVERED TO
Widley Farm New Down Lane 34 SPRING ROAD
Purbrook SOUTHAMPTON
WATERLOOVILLE
Hampshire 5019286
PO7 5SE
Pae1oft
mEm auanmiTy PRICE VALUE VAT
-l DESCRIPTION OF GOODS o e 3 oy
53815 [PULDNG SAND BULK BAG P e e B
eAd BAd
663469 [SUPAGROW TOPSOIL BULK BAG 600L. 2 6.1 4 2
eac] eacr|
Branch GOODS AMOUNT 2
EASTLEIGH TP
TRAVIS PERKINS TRADING CO, LTD
UNIT 16-17, PARHAM DRIVE VAT TOTAL &
EasLEiH ok o e
0238061 2781

Health & Safety: For infomation on products (e.g. COSHH please
TERMS NET MONTHLY visit wawtraviperkins,co.uk. Contac the HES Degt. during ofice
bours on (01604) 75242 i eta not aaieble.

Registered in England No. 733503, Registered Office : Lodge Way House, Lodge Way, Harlestone Road, Northampton, NNS 7UG.

Pay your account balance online at:
www.travisperkins.co.uk





 


 


 


                                                                                                                             


          


December 2023


 


 


Cover system validation report overview document, 31A North Street, Emsworth, PO10 7DA


 


 


  


 


Sirs


 


 


Parchow Groundworks have been advised that there is some confusion that may have been 


inadvertently caused by the report that we’d previously issued.


 


   


The purpose of this overview document is 


to explain the 


installation of the cover 


system


 


in terms 


sequential proce


ss, and 


where


 


appropriate, explain any 


deviation


 


from the 


cover system noted with 


in the GCC RMS, albeit 


the change being one of an 


enhanced


 


perform


ance


.


 


T


o 


aid 


understanding, the overview 


will deal with 


t


he bullet


 


points noted 


by the HBC Environmental 


Control officer and then proceed to describe the works process


 


to


 


better understand the installation 


of the cover system and to enable all stakeholders to 


have adequate comfort in i


ts efficacy and 


suitability for purpose.


 


 


 


Gar


den areas


 


 


The total garden areas given are accurate 


and 


indicate all areas that are subject 


to the specification 


shown in 4.3.2 of the GCC report ind


icating 


this.


 


This are


a 


is 190.53m2


. Th


is covers the areas with


in 


the gardens 


inclusive


 


of paths and patio


’


s etc


 


 


Conve


yance proof


 


 




                                                                                                                                               December 2023     Cover system validation report overview document, 31A North Street, Emsworth, PO10 7DA          Sirs     Parchow Groundworks have been advised that there is some confusion that may have been  inadvertently caused by the report that we’d previously issued.       The purpose of this overview document is  to explain the  installation of the cover  system   in terms  sequential proce ss, and  where   appropriate, explain any  deviation   from the  cover system noted with  in the GCC RMS, albeit  the change being one of an  enhanced   perform ance .   T o  aid  understanding, the overview  will deal with  t he bullet   points noted  by the HBC Environmental  Control officer and then proceed to describe the works process   to   better understand the installation  of the cover system and to enable all stakeholders to  have adequate comfort in i ts efficacy and  suitability for purpose.       Gar den areas     The total garden areas given are accurate  and  indicate all areas that are subject  to the specification  shown in 4.3.2 of the GCC report ind icating  this.   This are a  is 190.53m2 . Th is covers the areas with in  the gardens  inclusive   of paths and patio ’ s etc     Conve yance proof    

