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WORKS: SINGLE STOREY REAR EXTENSION TO FORM KITCHEN AND LIVING AREA
LOCATION: 14 LONE VALLEY – WATERLOOVILLE- PO7 5DZ          FOR: MARTIN SPENCER 
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All dimensions to be checked on site before the commencement of work and not scaled from drawings. Commencement of any works prior to the necessary Local Authority approval is entirely at the owner’s risk. 
The owners are to ensure that any requirements of the Party Wall Act are completed in advance. 

New rain water gutter run and connected to existing gutter that runs to existing rainwater down pipe.
Existing vent pipe replaced with new uPVC S&VP and connected to existing drain
Patio doors and brickwork removed and a new steel beam inserted encased for ½ hour fire protection and bearing a minimum 150mm on reinforced 300 x 100 x 65mm concrete padstones
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CONSTRUCTION NOTES
SUPPORT TO OPENINGS WHERE REAR AND INTERNAL WALL REMOVED: 
Rear external wall to the existing living room to be removed as shown and masonry and roof above supported on steel beam supported on padstones. Steel beam to be encased in timber framing with two layers of 9mm plasterboard and 7mm skim coat plaster to achieve minimum ½ hour fire resistance. Beam to bear on reinforced concrete padstones with minimum150mm bearings 

PLUMBING:
New waste from kitchen sink, washing machine and dishwasher to be upvc 32mm diameter waste with deep seal trap and rodding access at all changes of direction where applicable in accordance with BS EN2056 and Approved Document H. New waste run to new uPVC soil and vent pipe to replace the existing vent pipe, in the same location, and connected to existing drain run and inspection chamber.

RAINWATER DISPOSAL: New 100mm half round rainwater gutter to be fixed on brackets to fascia beneath roof slopes to match existing profile and laid to fall. Gutter to run and connect to existing gutter that runs and connects to existing 68mm dia. down-pipe discharging to stormwater drain. 
VENTILATION: 
Extractor hood above cooker in kitchen to have fan fitted to achieve minimum 30 litres per second extraction to external air.


Proposed Kitchen / Family Area
Existing Living Room
Existing Kitchen to convert to Study
5.3 m
Boundary Line
Chimney removed in conjunction with neighbouring property.

All kitchen waste to run to new S&VP 
Door and window and masonry below lintol removed and infilled to outer skin

image1.gif




image2.gif




image3.gif




