WORKS: SINGLE STOREY REAR EXTENSION TO FORM KITCHEN AND LIVING AREA
LOCATION: 14 LONE VALLEY – WATERLOOVILLE- PO7 5DZ          FOR: MARTIN SPENCER 
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All dimensions to be checked on site before the commencement of work and not scaled from drawings. Commencement of any works prior to the necessary Local Authority approval is entirely at the owner’s risk. 
The owners are to ensure that any requirements of the Party Wall Act are completed in advance. 
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CONSTRUCTION NOTES
FOUNDATIONS: 
Trench fill concrete foundations minimum 1.0m below ground level and to suit sub-soil, ground conditions, invert of drains and Building Control approval, minimum size 450mm wide x 850mm deep.

DAMP PROOF COURSE: 
Horizontal 100mm dpc’s to be minimum 150mm above all finished ground levels to external skin of wall, dpc and dpm to be well lapped together and to existing to form continuous moisture barrier. Cavities to continue 250mm below lowest dpc with vertical dpc’s provided at junction of new floor slab and perimeter walls and closed at reveals with insulated vertical ‘Damcor’ dpc’s.

EXTENSION WALLS: 
External skin of 103 facing brickwork to match existing, inner skin of 100mm Celcon standard blockwork and a 100mm cavity part infilled with 50mm Celotex CG 4000, blockwork finished internally with 3mm skim on 12.5mm lightweight plasterboard. Skins to be tied together with wall ties © 75mm centres horizontally and 450mm centres vertically and staggered and every block course within 300mm of external wall openings. Walls to achieve minimum 'U' value of 0.28 W/m2K.

BRICKWORK AND BLOCKWORK: 
All new brick and blockwork @ vertical junctions to existing walls to be well bonded or secured with propriety profiled stainless steel crocodile type system with a continuous cavity closed at opening reveals in insulation blockwork incorporating vertical dpc’s and closed at heads with non-combustible materials. Provide suitable ‘Catnic’ combined lintels/cavity tray (incorporating insulation materials) over external wall opening with min. 150mm end bearings and a min. of two weep holes per opening.




SECTION THRO0UGH EXTENSION at ‘B’ – ‘B’
SECTION THROUGH CONSTRUCTION at ‘B’ – ‘B’
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