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Scale of wooden stakes

ESC approached Chichester Harbour Conservancy for an approved contractor. The contractor was contacted and a quotation obtained. This provides a guide to the size of the stakes to be used. The original stakes providing erosion protection have rotted away this proposal provides a similar replacement.

[bookmark: _GoBack]The contractor’s quotation states:


Remedial Works At Bath Road

Wooden Stakes To Side Of Slipway

Based on 15 metres in length along line of original timber stakes

1. Supply, 150mm to 200mm diameter, wooden stakes. Drive stakes into bed of 
   foreshore on line of original timber stakes. Stakes to be 2.5 metres long and
   approximately 1 metre of stakes from water line to top of mud bank.

2. Clean mud off of slipway. Place mud behind new stakes.

3. Leave the area in a clean and tidy condition.

