0.5 m
Floor level
3.35 m
Ceiling joists run from back to front with firrings run to front of extension.
CONSTRUCTION NOTES
WARM DECK FLAT ROOF (UNVENTED): Formed with 3 layer built-up high performance felting to BS 747 & CoP 144, turned up a minimum 150mm under existing roof tiles with top layer covered in white spar chippings all bedded in hot bitumen laid over 85mm ‘Celotex’ EL 3000 insulation board (or similar) with a vapour control layer on 18mm marine ply roof-decking on firrings to min fall 1:60 fixed. 147 x 47mm C16 joists @ maximum 450 mm centres and a maximum clear span of 3.02m. Joists to be supported on 100 x 47 wall plate and joists hangers and strapped to perimeter walls at maximum 2000mm centres with 32 x 6mm galvanised mild steel straps. 
Roof to achieve minimum ‘U’ value of 0.25 W/m²K.

TIMBER FLOOR: New floor construction to achieve ‘U’ value of 0.20 W/m²K and to finish flush to existing floors formed of 25mm square edge floor grade boarding on 125 x 47mm joists @ maximum 400mm centres, with 120mm Celotex FR400 insulation sleeper walls @ maximum 1.8m centres with dpc and 97x47mm timber plate. Sleeper walls constructed on 100mm concrete over-site on 1200 gauge polythene dpm on sand blinded well consolidated hardcore base. The timber sub-floors walls and concrete slabs between joists, supported by honey-combed brick blinding to be tanked using cold-applied bitumen up to the DPC level. Void beneath to be ventilated with 225x75mm air-bricks to external air. 

WINDOWS: New Bi-fold doors, window and external door to be white uPVC double glazed unit with 16mm air gap and K glass or Argon filled sealed units all to achieve a minimum ‘U’ value of 1.3 W/m²K or better. Safety glass to be used in critical locations with opening doors and window to be a minimum 1/10th of room floor area and have 1/20th active opening vents and controllable trickle vent of minimum 8000mm². Doors and window to be sealed around junctions of frames and reveals in mastic. 
Permitted glazing; Proposed extension floor area (6.9 x 3) 20.7m² + (2.85 x 2.3) 6.56m² = 27.26m² x 25% = 6.81m². Area of existing openings built over - Patio doors (2.73 x 2.36) 6.44m², Rear kitchen window (1.05 x 1.1) 1.15m², Kitchen door (0.85 x 2.0) 1.7m². Total permissible glass = 16.1 m²
Proposed glazing; Bi fold doors (2.7 x 2.1) 5.67m² – Kitchen window (1.5 x 1.2) 1.8m² - Velux Flat roof Roof-light (1.2  x 0.9) 1.08m². Total proposed glazing = 8.55m². Glazing Permissible.


SECTION THROUGH EXTENSION at ‘A’ – ‘A’
SECTION THROUGH CONSTRUCTION at ‘A’ – ‘A’
– ‘B’


Ceiling joists run to side of extension with firrings run from back to front of extension. Joists supported on joist hangers hung from double joists bolted together. 
Floor joists run from back to front of extension.

Floor joists run from side of side of extension supported on joists hangers hung from double floor joists bolted together.
Min. 1 m below G/L 
Floor to ceiling height 2.5 m
0.85 m
Min. 0.45 m
All dimensions to be checked on site before the commencement of work and not scaled from drawings. Commencement of any works prior to the necessary Local Authority approval is entirely at the owner’s risk. 
The owners are to ensure that any requirements of the Party Wall Act are completed in advance. 

WORKS: SINGLE STOREY REAR EXTENSION TO FORM KITCHEN AND LIVING AREA
LOCATION: 14 LONE VALLEY – WATERLOOVILLE- PO7 5DZ         FOR: MARTIN SPENCER 
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