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	Dimensions(cm)
	Comments

	A

	H85
W185
L185
	Raised by 120mm to accommodate insulation for compliance with building regulations

	B
	H37
W110
L110

	Raised by 120mm to accommodate insulation for compliance with building regulations. Replaced with new dome.

	C
	H92
W198
L410

	No change

	D
	H76
W207
L290
	NEW INSTALLION OF SKY LIGHT

	E
	H78
W190
L292

	Raised by 120mm to accommodate insulation for compliance with building regulations

	F
	H67
W165
L250

	Raised by 120mm to accommodate insulation for compliance with building regulations

	G
	H86
W192
L192

	Raised by 120mm to accommodate insulation for compliance with building regulations
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