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Tel: (023) 9279 9741		Mobile: 07979 516 291
davidjones@solentindustrialroofingsystems.co.uk

Quote

10th May 2017

Mr Manish Patel
14 Leigh Road
Havant
PO9 2ET



Dear Manish

Thank you for your invitation to quote for the re-roofing of the flat roof on your property at the above address.
We would like to give you two systems of specifications for your choice:

System 1: Felt.

· Strip and remove approximately 70sm of damaged felt and decking this section of the roof to be re-decked with 18mm sterling board.

· The remainder of the existing felt roof covering to be stripped and removed of site in waste containers.

· Supply and install vapour barrier to the new and existing timber decking.
· 
· Supply and install 120mm insulation board to all areas fully bonded to vapour barrier.
· 
· Supply and install three layer felt system cap sheet to be of mineral finish.
· 
· Supply and install new GRP perimeter drip details.



·   All ridge tiles on the mono pithed perimeters to be removed and set aside for refitting.

· Supply and install 18mm sterling board to inner detail of the upstand allowing full encapsulation with felt system.

· Re-bed ridge tiles on completion.
 



System 2: Singly ply EPDM.

· Strip and remove approximately 70sm of damaged felt and decking this section of the roof to be re-decked with 18mm sterling board.

· The remainder of the existing felt roof covering to be stripped and removed from site in waste containers.

· Supply and install vapour barrier to the new and existing decking.

· Supply and install 120mm insulation board to all areas fully bonded to the vapour barrier.

· Supply and install single ply EPDM roof system to all areas fully bonded to the insulation.

· New steel plastisol coted trims to drip detail.
 
· All ridge tiles on the mono pitched perimeters to be removed and set aside for refitting

· Supply and install 18mm sterling board to the inner detail of the upstand allowing full encapsulation with the single ply system.

· Re-bed the ridge tiles on completion.



With both systems the existing upstands on the roof-lights will have to be raised up with timber to a minimum of 150mm above the new roof height.

The roof will be cut open allowing for the inclusion of a new roof –light in a new agreed position.

There are three roof-lights that will have to be removed and replaced with new lantern lights over the existing apertures, over the swimming pool area.

There is one roof-light that that may not need to be raised as the upstand appears sufficient.
 

The two smaller roof domes, one will be removed and boarded over; the second roof dome will be removed and raised up the new dome will be installed over the existing aperture.

Continued



All roof pipe penetrations will receive new chosen waterproofing applications.

All works will be carried out with manufactures installation instructions.





Associated works.

Rain water goods and facia boards.

· Remove and replace half round guttering and replace with new.
· Remove and replace facia boards with new.



Waste removal is included in our costs.



Cost for option 1                               £27,930.00     including Vat.

Cost for option 2                               £23,941.00    including  Vat.

Cost for facia and guttering            £1,680.00        including Vat.


Terms and conditions apply.







I hope this meets your requirements and look forward to hearing from you.


Yours sincerely



DAVID JONES
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