1 East Street Repairs and adaptations to South & West Elevations.
Health & Safety
An application will be made for pavement closures.
Given the location it may be necessary to engage a banksman when these works are undertaken.
Suitable warning notices indicating that work is in progress will be displayed, and where necessary barriers will be erected.
The height of some of the repairs will necessitate the use of a narrow platform tower.
Removal of existing signage and redundant fixings
Carefully remove all existing signage and discard to refuse site.
Carefully clean and re-fix and extend as necessary all surface water downpipe.
Remove coach lanterns, carry out off-site refurbishment, and reinstall. 
Carefully remove redundant surface cables.
Generally, remove foliage overhanging from first floor and treat surrounding area with weed killer.
Repairs to Brickwork
Attached photos will confirm the quantum of repairs required.
It is proposed that a propriety resin (Stonelux) be used as the material to fill the numerous old fixing apertures. Obtaining the correct colour match will entail obtaining samples of the product and preparing a sample repair for approval.
There is a considerable amount of staining on the brickwork, and this will be removed with a propriety brick cleaner.
Replacement bricks, missing bricks will be replaced to match the existing.
It is anticipated that the existing air vents will be replaced with new PVC grilles similar in design (see  drawing BR02). These grilles will be used to discharge air from the new ventilation system, and the route of the ducting is indicated on drawing BR01. The new grills are shown on drawing BR02.
Repointing Generally
Cut out and rake out loose mortar in joints. It may be necessary to use a battery driven small angle grinder. The joints are to be dust free prior to re-pointing.
The proposal is to provide a mortar mix as close in colour to what exists. It is not the intent to re-point the whole façade. A sample area of repair will be carried for approval by the Conservation Officer.
Decorations Generally
All loose and peeling paintwork is to be scraped off and rubbed down, where required propriety external filler will be used a stabiliser coat will be applied before treating with Black Sandtex smooth External Masonry paint.

