Conservatory Installation address;

11 Sherfield Avenue 
Havant

Hampshire 

PO9 5HT

Tree / Root Protection Plan

In order to ensure the safe guard and protection of tree’s the following precautions will be undertaken;
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Fencing is to be erected prior to any works

commencing, materials stored or associated 

machinery are present on site

The fencing will be maintained for the 

duration of the development unless otherwise 

agreed by the local authority
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No materials, chemicals or fuel shall be 

stored within the fence 

Correct and suitable signage will be 

provided and maintained throughout the

works 

Root protection areas will be pegged and marked out as defined in the relevant British Standard(s) to ensure trenches are avoided to these areas 
Method Statement for the removal of base foundation with surrounds the tree

The purpose of this statement is to protect any roots that may be beneath the foundations from damage thereby assuring the long term retention of the tree;

1. Pre commencement site meeting to be conducted to ensure all active construction members are aware of the requirements of tree protection

2. Ensure fencing has been installed in accordance with the tree protection plan

3. Only hand operated tools are to be used for the removal of the foundations. No wheeled or tracked excavators are to be used

4. The existing ground surface and foundation depth is to be broken up in sections sequentially away from the tree

5. All debris is to be removed from the area by hand only. No wheeled or tracked excavators are to be used

6. Once existing ground foundation has been removed, review area for presence of roots prior to continuing excavation works
Method Statement for Root Protection
The purpose of this statement is in the event of any roots being found in excess of 20mm diameter to ensure the long term protection of the root and tree;

1. The use of a air spade shall be utilised to expose the root area

2. Once exposed any pruning necessary will be undertaken in accordance with BS3998:2010 recommendations

3. Suitable permable root guard barriers shall be installed
4. The root guard barrier shall be surrounded with 100mm deep composted wood chipping to allow for further potential growth

5. Once the root is protected as 2, 3 & 4 the area shall be dressed with top soil

6. In the event of the root location affecting the install, guidance shall be sought from a suitably qualified person prior to continuing

General Note

Site supervision will be maintained and monitored whilst excavation works are being undertaken by our Local Installation Field Manager and the above details adhered too. Once the pre commencement site meeting has been arranged we would be able to disclose the date to the council so should the tree officer or case officer wish to attend to discuss the protection plan further. 
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PROTECTIVE FENCING. THIS
FENCING MUST BE
MAINTAINED IN ACCORDANCE

WITH THE APPROVED PLANS
AND DRAWINGS FOR THIS
DEVELOPMENT.

TREE PROTECTION AREA

KEEP OUT!

(TOWN & COUNTRY PLANNING ACT 1990)

TREES ENCLOSED BY THIS FENCE ARE PROTECTED BY
PLANNING CONDITIONS AND/OR ARE THE SUBJECTS OF A
TREE PRESERVATION ORDER.
CONTRAVENTION OF A TREE PRESERVATION ORDER MAY
LEAD TO CRIMINAL PROSECUTION

ANY INCURSION INTO THE PROTECTED AREA MUST BE
WITH THE WRITTEN PERMISSION OF THE LOCAL
PLANNING AUTHORITY







