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Method statements accompanying drawing 
1. Three in number 225 x 50 mm timber bearers are to be secured to the inside face of twittens wall as per drawings 
2. Scaffold tubing is to be braced against the bearers and cantilevered into cast concrete padstones set into the ground 
3. Additional tubing is to be cross braced and attached to the diagonal bracing 
4. Once construction begins on the dwelling the eastern elevation rat-trap wall to be taken down and raked back leaving a 45degree portion of the wall in tacked providing additional support for the twittens wall 
5. A same approach to the post 1974 curved wall to the western elevation is to be adopted during the construction process 
6. Once the archeological proposal has been agreed and implemented herris panels will be clipped inside the wall bracing giving a 100mm void between the twittens wall and the protection .
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1 Thre i umber 225 » 50 i tmber earers re tobe
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