


Ventilation/Extraction specification
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1) 4500mm x 1000 canopy hood

2) 1 x tcbb 500 turbo prop fan motor 

3) 1 x 500 dia silencer to reduce noise levels -10dba 

4) carbon filtration system 

5). Fresh air Ventillation system 

6)  fitted above canopy 

7). 2 x Speed controller for both fan motors 

8). Interconnecting ductwork 




