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Glazed sides to be added to the walkway “ bridge” only. The existing balustrade to be removed and replaced with glazed sides. Length approx 9.5 M long and 2.4 M high
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