Fencing Havant@GrowingPlaces

We intend to install GuardSAFE Vmesh Security Fencing to create a secure area for the Nursery Children. 
The posts will be 620mm into the ground, all other specifications and dimensions are below.
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image2.jpg
= =

Suitable For:

® New Build Housing

e Commercial Development
e Schools

® Hospitals

Key Features:

® Attractive Design

e Available from Stock
o Cost Effective

® Unobtrusive Design

Product Finishes:

Other RAL

6005 8§ 9005 X 4 & colour finishes
y available
Quality Guarantee Nationwide Delivery Large Order Discount Dedicated Customer Service
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Produced from Galvanised Wire to BS EN 10244-2:2001 Class D
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Post material manufactured to BS EN 10210-2: 1997 and galvanised
D to BS EN 10345:2009

D Both panels & posts are powder coated to BS EN 13438: 2005
(minimum 100 microns)

The Vmesh mesh system is easy to
install and it is supplied complete
with metal clips and M8 Security
fixings which require a security tool
to install. The panels can be stepped
on site to help the fenceline follow
the ground.

Quality Guarantee Nationwide Delivery Large Order Discount Dedicated Customer Service




