Padnell Avenue Job Specification 
T1 – Oak tree: Reduce south east facing canopy by 1.0 metres or to nearest growth point. Leaving a 12 metre canopy in diameter remaining. 
T2 – Oak Tree: No work required 
T3 – Oak Tree: Reduce south east facing canopy by 1.0m or to nearest growth point. Leaving a 8.0 metre canopy in diameter. 
T4 – Oak Tree: Crown raise to 5.0m on south east side. Reduce south east facing canopy by 2.0 metres or to nearest growth point. Leaving 12.0 metre canopy in diameter. 
T5 – Oak Tree: Crown raise to 5.0m on south east side. Reduce south east facing canopy by 1.0 metres. Leaving a 13.0 metre canopy in diameter. 
T6 – Oak Tree: Reduce south east facing canopy by 1.0 metre. Leaving a 10 metre canopy in diameter. 
T7 – Oak Tree: Crown raise to 5.0 metres on south east side. Reduce south east facing canopy by 1.0m. Leaving a 10 metre canopy in diameter.
T8 – Oak Tree: Crown raise to 5.0 metres on south east side. Reduce south east facing canopy by 2.5m or to nearest growth point. Leaving a 12.5 metre canopy in diameter.
T9 – Oak Tree: No work required 
T10 – Oak Tree: Crown raise to 5.0 metre on south east side. Reduce south east facing canopy by 2.0 metres or to nearest growth point. Leaving a 10 metre canopy in diameter.
T11 – Ash Sapling: Remove to ground level. 
T12 – Oak Tree: Reduce south east facing canopy by 1.0 metre. Leaving a 7.0 metre canopy in diameter. 
T13 – Oak Tree: Reduce south east facing canopy by 2.0m. Leaving a 9.0 metre canopy in diameter. 
T14 – Oak Tree: Reduce south east facing canopy by 2.0m. Leaving a 10 metre canopy in diameter. 
