Construction Environment Management plan

For

 Installation of 3 No. Covered and Partially Enclosed Padel Courts with Associated Lighting, Noise Ecological Mitigation Measures

Introduction

This CEMP is to provide detail for approval of the proposed measures that will be put in place for the duration of the construction project and adhered to at all times.
  This includes
· Parking for Site Operatives and Visitors
· Loading and unloading of plant and materials
· Storage of plant and Materials
· Erection and maintenance of security fencing
· Provision of Wheel wash facilities
· Dust and dirt suppression during construction
· Turning vehicles on site 
· Location and provision of Site facilities 

Site layout plans
Find attached (drawing A109) a site layout showing the location of storage, welfare WC, and skip

Project description
The project is to Install 3 No. Covered and Partially Enclosed Padel Courts with Associated Lighting, Noise Ecological Mitigation Measures

Environmental impacts and management 
The build is expected to take around 12- 16 weeks during that time the following measures will be put in place to address the concerns listed 

Use of fences and barriers to protect adjacent land
The extent of the perimeter of the two open sides of the site and the storage compound will be secured with fixed Heras fencing as indicated in green on the accompanying CEMP site plan. This will make the site safe, secure and avoid the possibility of unauthorized people straying onto this area. Gates to the fenced areas will be chained and padlocked when the site is not in use for construction and will be regularly monitored. The rear of the site is already secure with a 3.8m metal fence.


Storage of Materials 
Structural steel will be delivered to the construction area as needed for immediate use and thus will not be stored for any period on site. Other materials such as insulated cladding /roofing and fittings will be stored in the materials storage area shown in on the CEMP site plan and will be covered as necessary to avoid water and wind damage.

Dust reduction
Particular care will be taken to maintain dust emissions at a practicable minimum when working. Best practice mitigation will be followed during dry conditions, 
Dust reduction measures will include: 
· The careful management of any required sand and gravel so it is delivered to site on an as needed basis.
· The sheeting of such loose materials on site. 
· Ensure all delivery vehicles stay on the road to avoid bringing dirt onto the public highway.
· Ensure that any area where plant and machinery is operating, is dampened with a fine spray of water in dry conditions.
· visual monitoring will be carried out on a daily basis during works to assess the requirement for dust suppression by water spray.  
No groundworks or construction will commence on site before a suitable and adequate water supply has been provided & made available for use in the mitigation of construction impacts. 
Toilet facilities,
Toilets will be provided as shown on the accompanying CEMP site plan for use by the construction operatives whilst work is in progress.

Management of construction waste on site
A covered (netted) skip will be provided as required to contain construction waste; this will be replaced whenever full. And will be kept in the designated area as shown on the accompanying CEMP site plan
The site will be inspected daily and a strict no litter policy will be enforced with bins provided nearby to working operatives that will be emptied to the skip located as indicated on the plan.

Noise and vibration
Due to the nature of the project and the limited requirement for ground works the emission of noise & vibration will be limited, and there will be no percussive piling, use of heavy machinery will be no more than is usual in the day to day operation of the existing site. However this will be monitored and controlled if required.

Parking on site
A parking area for operatives and visitors together with a vehicle turning area will be provided on site
These are shown on the accompanying CEMP site plan 

Unloading of plant and machinery
Whilst the majority of any plant required is already available on site, should any additional plant be delivered, it will be off loaded in the yard clear of the public highway

Deliveries
Deliveries will be made to the material storage area or main site with room being provided as per the CEMP site plan for stopping and turning. When reversing a banksman will ensure the space is clear and will direct the vehicle

Wheel cleaning
Due to surface materials, the layout of the site and surrounding area no vehicle should need to leave the surfaced concrete area and as such should not collect dirt and mud on its wheels. A hose and cleaning brush will be provided on site to ensure any tools or plant is cleaned before leaving site on any open transport such as a trailer
Conclusion.
We believe the listed measures will ensure the project has minimal impact on the surrounding land and natural environment. This development will be undertaken in a considered, clean and professional manner with all stipulations by the planning authority adhered to.
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