Jane Mottershead Designs Limited
Email: jbmottershead@aol.com

FLOOD RISK ASSESSMENT

39, Eastoke Avenue, Hayling Island, PO11 9QW

Proposed extension and roof alterations to existing bungalow.

Sequential Test

This application is for an extension of under 250 square metres to an existing dwelling, so is a minor development.
Flood Proofing/resilience and resistance techniques will be included into the proposal in accordance with ‘Improving the flood performance of new dwellings’ CLG (2007).
A Minor Development in a Flood Zone.

The floor levels of the proposed extension will be set at the same height as the existing floor levels.
The ground floor will be constructed to be resistant against flooding.
The ground floor will be built with a suspended concrete floor, all new walls on the ground floor will be constructed out of lightweight block’s.  Subject to Building Control approval and the applicant’s Structural Engineers recommendation, added improvements such as an extended concrete footing, a waterproof membrane laid in the foundations, a raised d.p.c. and closed cell cavity insulation, will be included wherever possible. 

Where air bricks are installed, they will be fitted with a removable cover.

Anti-backflow valves will be fitted to drains and sewers.

The boiler and hot water cylinders will be situated off ground floor level.
All electrical services will be connected at high level and brought down through the ceilings where possible.
Wherever possible rainwater will be collected in water butts and used for watering the garden.

