
HAVANT BOROUGH COUNCIL

	APPLICATION No.
	APP/23/00417

	LOCATION
	The Pavilion and Recreation Ground, Horndean Road, Emsworth, PO10 7PT

	PROPOSAL
	Installation of shipping container.

	RECOMMENDATION

	No objection, subject to conditions

	DATE

	5th July 2023



Reasons for Recommendation
The Council seeks to protect tree coverage in the Borough, sympathetically incorporating existing features into the overall design of the scheme including measures taken to ensure their continued survival. 

The applicant has sought to work with the authority to determine a suitable location that provides for the specific development needs and proximity to facilities with suitable access, whilst also taking account of the impact on the mature trees within the recreation ground. 

The additional information submitted by the applicant has sought to clarify the limited impact the development will have to the adjacent mature trees. Whilst the information submitted is very limited there is an obvious intention to respond to initial comments from the authority that raised concerns of the development being potentially within the root protection area of the adjacent trees. The applicant has amended the development so that the shipping container will placed above ground level on wooden sleepers to allow the aeration of the soil, therefore minimising impact to the root protection area of the tree. 

Based on the measures proposed by the applicant, if the officer was minded to grant permission the potential impact of the surrounding trees should be secured by way of condition, and would be in accordance with Policy CS16 and DM8 of the Havant Core Strategy (2011).

Recommendation:
Approval subject to the following conditions;
a) Pruning works: 
Any required tree works shall be pruned in accordance with the recommendations in British Standard BS3998:2010 (Recommendations for Tree work).
Reason:  To ensure the continuity of amenity value afforded by the trees in question and having due regard to policies CS16 and DM8 of the Havant Borough Core Strategy (2011) and the National Planning Policy Framework.

b) Tree protection measures:
No development, including site clearance, shall extend beyond the red outline of the container shown in the ‘Emsworth Park Copy’ Site plan (dated 2023-06-28 14:03:45). If development did extend beyond this boundary a dimensioned tree protection plan in accordance with Section 5.5 and an impact and method statement detailing precautions to minimise damage to trees in accordance with Section 6.1 of British Standard BS5837: 2012 (Trees in relation to design, demolition and construction - Recommendations) must have been submitted to and approved in writing by the Local Planning Authority prior to commencement.
Reason: To safeguard the continued health and presence of such existing vegetation and protect the amenities of the locality and having due regard to policies CS16 and DM8 of the Havant Borough Core Strategy (2011) and the National Planning Policy Framework.

c) Foundations:
No dig construction must result in the shipping container being located above ground level in the location shown on ‘Emsworth Park Copy’ Site plan (dated 2023-06-28 14:03:45. If additional foundation details were required no works shall commence until details of special foundations that will be able to 'bridge' the rooting areas of trees or foundations that can be inserted through the root system without causing harm to the neighbouring trees must have been submitted to and approved in writing by the Local Planning Authority. The development shall be implemented and thereafter maintained in accordance with the approved details.
Reason: To safeguard the continued health and presence of such existing trees and protect the amenities of the locality and having due regard to policies CS16 and DM8 of the Havant Borough Core Strategy (2011) and the National Planning Policy Framework.

d) Tree Protection: Foundations - Hand digging excavations:
Any excavation work, including foundations, within the existing root protection area of the neighbouring trees shall be carried out only by hand in accordance with the BS:5837:2012 'Trees in relation to design, demolition and construction Recommendations'. Any roots over 25mm in diameter shall not be severed and if exposed should be packed with sphagnum moss and wrapped with hessian to prevent the entry of rot causing fungi and micro-organisms. No roots shall be left exposed to the air, water, snow or frost for more than two hours without appropriate protection.
Reason:  To ensure the trees are not adversely affected by the construction of the development and having due regard to policies CS16 and DM8 of the Havant Core Strategy (2011) and the National Planning Policy Framework.

