[image: ]



	For the attention of Mr D Eaves
Planning Development
Havant Borough Council
Public Service Plaza
Civic Centre Road
Havant 
Hampshire
PO9 2AX


	Hampshire Fire and Rescue Service HQ
Business Fire Safety
Leigh Road,
Eastleigh
Hampshire
SO50 9SJ

Tel:  023 8062 6751
     Email: csprotection.admin@hantsfire.gov.uk




Date:	<-22 June 2018->

Enquiries To:	Sailesh Parmar	My Reference:	F6/SP/<<-00831149->>

Mobile Tel:                           	Your Reference:	APP/18/00234


Dear Mr D Eaves

Town & Country Planning Act 1990
Fire and Rescue Services Act 2004
Planning Application Number: APP/18/00234
Wellington Way, Waterlooville, Hampshire

Drawings and Documents Referenced
	Title
	Project Ref
	Drawing No
	Revision
	Date

	Site Plan
	Wellington Way
	02
	E
	21/12/17



Description of Works:

HFRS understands that the project involves the Demolition of existing shopping parade and redevelopment of the site to provide a nine-storey building consisting of 264 No. 1 bed/studio build to rent apartments and associated amenity facilities, an A2 unit (Financial and Professional Services) together with associated parking and landscaping

I confirm that Hampshire Fire and Rescue Service (HFRS) has received your application, dated 12 June 2018. The inspector named above has considered the information provided and has made the following comments:
Building Regulations: Access for Firefighting
Access and facilities for Fire Service Appliances and Firefighters should be in accordance with Approved Document B5 of the current Building Regulations. 


Hampshire Act 1983 Section 12 – Access for Fire Service
Access to the proposed site should be in accordance with Hampshire Act 1983 Sect, 12 (Access to buildings within the site will be dealt with as part of the building regulations application at a later stage).  Access roads to the site should be in accordance with Approved Document B5 of the current Building Regulations. 
Fire and Rescue Services Act 2004
The following recommendations are advisory only and do not form part of any current legal requirement of this Authority. 
Access for High-reach Appliances 
High reach appliances currently operated by the HFRS exceed the maximum requirements given in Section 17 of the Approved Document B.  When considering high rise buildings these variations should be considered as additions and incorporated as follows.  Structures such as bridges, which a high-reach appliance may need to cross should have a maximum carrying capacity of 26 tonnes.  Where the operation of a high reach vehicle is envisaged, a road or hard standing is required 6m wide.  In addition, the road or hard standing needs to be positioned so that its nearer edge is not less than 3m from the face of the building. 
Water Supplies 
Additional water supplies for fire fighting may be necessary.  You should contact the Community Response Support, Hampshire Fire and Rescue Headquarters, Leigh Road, Eastleigh, SO50 9SJ (risk.information@hantsfire.gov.uk) to discuss your proposals.
Fire Protection 
HFRS would strongly recommend that consideration is given to installation of an Automatic Water Fire Suppression Systems (AWFSS) to promote life safety and property protection within the premises. 
HFRS is fully committed to promoting Fire Protection Systems for both business and domestic premises.  Support is offered to assist all in achieving a reduction of loss of life and the impact of fire on the wider community.->
Testing of Fire Safety Systems
HFRS strongly recommends that, upon commissioning, all fire safety systems are fully justified, fully tested and shown to be working as designed.  Thereafter, their effectiveness should be reconfirmed periodically throughout their working lifecycles.
Fire-fighting and the Environment
Should a serious unsuppressed fire occur on the premises, the water environment may become polluted with ‘fire water run-off’ that may include foam. The Service will liaise with the Environment Agency at any incident where they are in attendance and under certain circumstances, where there is a serious risk to the environment, a ‘controlled burn’ may take place.  This of course could lead to the total loss of the building and its contents.

Premises’ occupiers have a duty to prevent and mitigate damage to the water environment from ‘fire water run off’ and other spillages.

Timber-framed Buildings
These types of buildings are particularly vulnerable to severe fire damage and fire spread during the construction phase.

The UK Timber Frame Association publication '16 Steps to Fire Safety on Timber Frame Construction Sites' provides guidance on this issue and is available from: 
http://www.ttf.co.uk/Document/Default.aspx?DocumentUid=E588E0CB-0873-4038-BF4A-B8F83681CB7F
This guidance should be read in conjunction with the 'Joint Code of Practice on the Protection from Fire of Construction Sites and Buildings Undergoing Renovation', published by the Construction Confederation and The Fire Protection Association (Sixth Edition, ISBN 1-902790-33-2)
Copies of the 'Joint Codes of Practice' and useful sister publication, 'Construction Site Fire Prevention Checklist' (Second edition, ISBN 1-902790-32-4), are available for purchase from the Fire Protection Association
(www.thefpa.co.uk ) 
and from the Construction Industry Press 
(Publications for Construction Professionals and Builders | CIP Books)
If have any queries concerning these matters may be directed to the inspector named above but all correspondence should be addressed to the Chief Officer.

Please quote our reference number on all correspondence.

Yours sincerely



Neil Odin
Chief Officer 
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