Technical specifications of proposed LED solar street lighting

	LED Lamp Units
	

	Maximum Size
	1000(L)*300(W)*250 (T) mm

	Maximum lamp power 
	80 watts

	Maximum Luminous Flux 
	3000 Lumen 

	Maximum horizontal Illuminance (Across whole site)
	40 Lux across 375 sq metre MUGA site 

	Maximum hours of operation 
	6 hours daily (3pm-9pm).  

	Solar Panels
	

	Maximum Size 
	1500(L)*1500(W)*250 (T) mm

	Maximum Photovoltaic Power 
	200 watts

	Columns
	

	Column height
	5m minimum / 8m maximum

	Minimum distance of installation
	15m separation

	Battery
	

	Component and battery storage
	Above ground cabinet

	Battery 
	Lithium 60 AH capacity (Max)
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