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Bunting Gardens - Schedule of Proposed External Materials
	Location

	Material

	New footpaths (Highways)
	Asphalt concrete paving in accordance with with HCC Specification (Hampshire County Council Model Documents), The National Specification for Highways Works (SHW) Series 800 and BS EN 13108-1


	Parking Areas
(Highways)
	Asphalt concrete paving in accordance with with HCC Specification (Hampshire County Council Model Documents), The National Specification for Highways Works (SHW) Series 800 and BS EN 13108-1


	Tactile Paving
(Highways)
	Concrete Tactile Flag Paving - Tobermore Corduroy, colour; buff.


	Kerbs and Edgings
(Highways)

	Standard precast concrete kerbs and edgings to BS EN 1340

	Road markings to demarcate parking bays
(Highways)
	White thermoplastic paint system to Road Safety Markings Association standard specification document for road marking and road studs (StanSpec).


	Footpaths, front gardens and patios
(non-highway)
	Concrete Flag Paving - Tobermore Textured Paving Slabs, colour: natural.
With concrete sett feature elements - Tobermore Pedesta, colour; natural.


	Walls (garden walls  and house walls)

	Brickwork - Ibstock Coleridge Yellow Multi

	Railings and guardings to front gardens
	Galvanised steel to BS EN ISO 1461 and powder coated to BS 1722-16, colour; black


	Windows & Patio Doors
	Composite aluminium clad timber windows - Nordan NTech Villa, colour; Window Grey RAL 7040


	Window Cills

	Cast concrete cills - Forticrete Stooled Ciff Ref T1-40, colour; Portland


	Front Doors
	Nordan HomeGuard, colour Window Grey RAL 7040


	Roof
	Concrete interlocking tiles - Marley Duo Edgemere, colour; Smooth Brown


	Rainwater Goods
	Aluminium box gutters and rainwater pipes - Dales Delta 200 & 150, with Square Contemporary rainwater pipes, colour; RAL 7040


	Fencing
	Pressure treated softwood close-boarded fences




