Construction Environmental Management Plan (CEMP)
For balcony at
90a Southwood Rd Hayling Island PO11 9QF
APP/21/00586  Erection of purpose built balcony approx. 6m long (along face of building) by 2m wide (extending from face of building), positioned on the south elevation of 90a Southwood Rd, Hayling Island PO11 9QF     21.0672
With reference to the consultee comments from Natural England and the County Ecologist (see link below), the following plan is to mitigate any potential harm and noise disturbance to overwintering birds on the beach in front of the property (C19; Primary Support Area), that might be caused by construction of the balcony.
https://planningpublicaccess.havant.gov.uk/online-applications/applicationDetails.do?activeTab=documents&keyVal=DCAPR_250969 
As a keen supporter of conservation myself, I fully respect the need to protect wildlife.  The plan to mitigate this potential noise problem in constructing the proposed balcony includes:
1. The balcony will not be constructed between 1st October and 31st March, so as not to disturb the overwintering birds.
2. Most of the construction of the balcony will occur offsite, so drilling and fixing the parts will be minimal near the area of the beach. The large parts will be transported and put together at the site.
3. Impact criteria to address as requested by Natural England: 
• Noise/visual/vibrational impacts – I have discussed this with the builder and they do not envisage noise exceeding 69db.  Regarding ground vibration when digging holes in the ground for the padstones, the work will not take place between October-March and will not take long on the one day of construction.  
[bookmark: _GoBack]• Visual screening (for SPA birds) – the digger and activity will only occur on one day, so visual screening is not necessary.
• Storage of construction materials/chemicals and equipment – the work will take place within the same day, so no storage of materials will be necessary. There will be no chemicals involved
• Dust suppression – any dust from digging into the ground or drilling into walls will be dampened down by hosing with water. 
• Chemical and/or fuel run-off from construction into designated sites – not applicable
• Waste disposal – material (gravel/pebbles/debris) extracted from the ground for placing the padstones will be re-distributed across the site (garden area is of pebbles, boarded by flower beds) and dampened down in the process. This will be the same process as when the patio was constructed (which was on a larger scale). All other waste packaging etc will be removed from site by the builder. 
Although we would obviously like the balcony to be in place as soon as possible, we understand and accept that if planning permission cannot be processed and approved in time to enable the construction to take place before 30th September 2021, we will not attempt to do the work over winter.  
Mary Stokes
25th August 2021
