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Picus Sonic Tomographic Test Report
Tests undertaken: 14th August 2015 by Mr Kim Gifford. In the area of test and at the time of inspection.
Method: using Picus software Q72std, 10 modules in accordance with manufacturers manual. 
Brief: Provide Picus Tomographic Testing analysis and reports as follows
.
Site: 39 Roger mead Hayling Island
 
1. Picus Test : Walnut
See attached image:
Test . level: 150cms  approximately from ground level.
Picus Test Analysis: The Tomographic image shows  decay evident adjacent to test points  6,7,8,9 by old pruning wound.
 
Recommendations: Remove whole specimen because of the extensive decay present.
 
If you require any further information please do not hesitate to contact me. 
 
Kind Regards
 
Kim
 
Kim Gifford
Gifford Tree Service
 
www.treetesting.com 
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