HAVANT  BOROUGH  COUNCIL
MEMORANDUM
	From:
Environmental Health
	To:         Development Services Manager

	
	FAO:      Mrs Sally Smith      

	Our Ref:
EH/LTG/ltg
	Your Ref:      APP/13/00020

	
	

	Ext. No:
446668
	Date:  8 February 2013           


Re: Land and garden north of 1 Leigh Cottages, Petersfield Road, Havant, PO9 2HT
Erection of 1No. 3 bed house with new pedestrian and vehicular access from service road off Martin Road.  (Revised application.)

I refer to the above application under the Town & Country Planning Acts passed to this Service for comment.

I still have some difficulties with this latest application and whilst the applicant has clearly now looked at the document “Calculation of Road Traffic Noise” published by the Department of Transport in 1988, and PPG24 (now revoked), she still has not addressed the issue that it cannot be said that traffic at this location in Petersfield Road is free flowing. In view of the stop/start nature of traffic at this site in such close proximity to a traffic light controlled junction, I believe the only way that an accurate assessment of noise levels at the site could be made with any degree of confidence would be to measure it over a 24 hour period.

Having said that, I can see that the architect has gone out of their way to come up with a layout which uses non habitable rooms such as the kitchen and bathrooms to shield the habitable rooms from traffic noise from Petersfield Road, and I do not doubt an acceptable internal noise environment could be achieved. Indeed, the proposed layout of rooms is a model which we would be pleased if other developers were to emulate. 
However, to work out what specific measures, such as double glazing, would be required to achieve a desirable internal noise level it would be necessary to know the precise external noise level. The other alternative would be to specify a glazing configuration and ventilation package that errs on the side of caution.
I would therefore ask that if consent is granted the following conditions be attached:

(i) Details of measures to control external noise.
The development hereby permitted shall not commence until a scheme for protecting the proposed dwelling from traffic noise from Petersfield Road has been submitted to and approved in writing by the Local Planning Authority.  The dwelling shall not be brought into use until the implementation of all works forming part of such approved noise protection scheme has been completed in full accordance with all detailed components of such scheme.

N.B. Maximum noise level (predicted 15 years from completion of dwelling) in habitable rooms, with windows closed and other means of ventilation provided:

     Daytime          

35 dB LAeq,16h
     Night time        
30 dB LAeq,8h
    Reason:  To safeguard the amenities of occupiers of those dwellings. 

I would anticipate that it would be sufficient to achieve this standard by ensuring that habitable rooms with windows on the north or south facades be double glazed with a minimum glazing configuration of 6: 6-20: 4, i.e. two panes of glass 6mm and 4mm thick separated by a gap of between 6 and 20mm. Any habitable room on these façades without an openable window on the rear façade (i.e. not dual aspect) would need to have a means of acoustically insulated ventilation provided so that the windows can be kept closed.


(ii) A separate condition should be applied to ensure the existing brick/stone wall fronting Petersfield Road and along the northern boundary of the site are retained and maintained as part of any noise protection scheme.
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L.T. Glass

Environmental Health Team Leader (Environment)
