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Tree Report

Monlas, Northwood lane. Hayling Island, Hampshire. PO11 OLR

Location of trees -
See sketch map

No trees with a stem diameter of 150mm or under have been included as a part of
this report. Also hedging Conifers and other assorted small trees and shrubs have
not been included in this report.
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Trees -
Tree no. 1 2 3 4
Species Weeping willow | False Acacia Ash Macrocarpa
Height (M) 8 12 8 12
Stem Diameterat | 650 400 250 700
1.5m above ground
level (mm)
Branch Spread at |3.5,4.7,47,39 |34,10,35,2 [4,4,4,32 3,6,55,6
compass points N E
SW (M)
Crown clearance |3 3 25 3
Age Class Mature Mature Middle ages Mature
Physiological Fair Poor Poor Fair
condition
Structural condition | Leaning to E. Leaning to E 4 stemmed from | 3 stemmed from
Recently reduced | causing ground | ground ground.
due to wind heave.
damage
Estimate years 15+ 10 15+ 15+

remaining

Quality and Value

Low quality and
value
(10yrs+)

Low quality and
Value
(10yrs+)

Low quality and
Value
(10yrs+)

Low quality and
Value
(10yrs +)

Recommendations

Reduce
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TPQ’s / Conservation area - Hampshire
None of the trees are protected by tree preservation orders and the site is not PO11 OLR
within a conservation area. 02392 469039
07845 367063

www.jptrees.co.uk

Effect of development on amenity value -
None of the trees will be affected by the proposed development, so therefore a
change in amenity value would not be applicable.

Tree protection -

In accordance with the proposal, damage to the root area would not be applicable
as the existing surface areas within the root protection zones are not to change.
The existing driveway surface will be retained where it runs within a root protection
zone.

To protect the trees heras fencing supported on posts driven into the ground will be
used on the site in the positions shown on the sketch map.

The protection will be installed prior to any demolition or works commencing and
will be maintained throughout building operations. Signs will be attached to the
fencing stating clearly that this fencing is for tree protection and must not be moved
without authorization.

Tree works -
Any pruning will be undertaken in accordance with BS3998:2010
‘Recommendations for Tree Works’





