Design and Access Statement 53 Wheatlands Avenue Hayling Island
Project

2 Storey side extension front porch and replacement of flat roof with pitched mansard roof

Site 

The property is a three bedroom detached house which is in a somewhat dilapidated condition with some internal and external walls removed for potential possible work which has never been undertaken, these include the 1m parapet wall to the flat roof which for the purposes of street scenes etc does show the buildings height in existing drawings as 1m lower than it was before the parapet wall was temporarily removed.
The property is a three bedroom property with living accommodation at first floor level and bedrooms and bathroom at ground floor level, it is set back 6 m from the highway and is screened on all sides by hedging and fencing The site is approx 0.04 h and has a double garage to the rear. Wheatlands Avenue is a long wide road running East West and No 53 is situated on the North side at the eastern end adjacent to number 5 Bosmere Road at the corner of the junction
The properties in Wheatlands Avenue have evolved randomly over a period of time and are a mixture of sizes styles and material types as are many in the area. Originally the properties were small dwellings on generous 15m wide plots, however most (but not all) have been redeveloped with a mixture of detached bungalows chalet bungalows and houses, in some cases plots have been subdivided to form semi detached properties.
No 53 and No 5 on the corner were built in a similar 1930s style design with external stair cases to a terrace at roof level surrounded by a parapet wall. 

Context and Design
This site has been subject to a previous application in 2011 ref APP/11/00014 which was refused on the grounds bulk and height being detrimental to the street scene.

To resolve these problems detailed discussions and revised designs where discussed with the planning team involving David Eaves, Senior Planning Officer and Adele Maher Urban Designer.

These resulted in a view that the planning objections could be addressed by a revised design based around an alternative option (Option 4)  The new proposal is based around option 4 and has made further efforts to reduce ridge height etc 

The design has lowered the ridge height by utilizing a hidden mansard roof it has removed roof lights from the roof structure, it has incorporated hips to the roofs to reduce the impact of the roof and porch, it has set back the side extension and reduced the height of the side extension roof to make it subservient to the main building.

The proposal is now very close to the ridge height of number 5 and the original parapet height of no 53 before the parapet was removed and follows the principles agreed with the planning and urban design officers. (see attached email from David Eaves (Senior Planning Officer)

The design will keep the three bedrooms at ground floor level and provide a drive through garage, at first floor level the living accommodation will be expanded in an open plan format to provide additional space.

Materials

What remains of the existing rendering is in extremely poor condition and will need removal, the design aims to re render the first floor and then use blue grey Marley Eternit fibre cement weatherboard to the first floor with white pvc windows and edging to apertures, this will aid the breakdown of the mass of the building and is in context with the diversity of the street scene and other properties within the sandy point beach side area. The roof will be slate/ slate look alike to match the weatherboard style utilized in the design. Again these materials have been discussed as been acceptable with the Urban Designer.

As Requested detailed street scene images have been created in an accurate building information model to demonstrate the building within the street scene.

Access and Landscaping

The site is level and suitable for access for disabled persons. The Gardens offer some scope for planting and landscaping which will be undertaken once the building work is completed.

