ADDENDUM 
 
PLANNING COMMITTEE 
DATE 9th April 2026 
 
APP/25/01015 – Part retention of ground floor commercial unit (Use Class E); conversion of remainder of ground floor and first floor to form 8 x 1 bed flats (Use Class C3); construction of 2nd floor with recessed 3rd floor mansard roof to form 12 bed Shared Living Property (HMO - Sui Generis); with associated parking, refuse and landscaping.
212-218 London Road, Waterlooville, PO7 7AJ

Updates to Officer Report
The following updates, comprising minor corrections in respect of the officer report, an additional Environmental Health comment, and an amendment to a condition are as follows:

Typographical Correction
Section 7 under Habitats Regulations Assessment & Appropriate Assessment, under both Recreational Pressure and Water Quality the report erroneously states the applicant has entered into a legal agreement to secure the mitigation package. The legal agreement has not yet been signed and its completion forms Recommendation A at section 9 of the report. These two sentences at Section 7 should be deleted from the report. 

Additional Environmental Health Comment received:
The additional Environmental Health comment received is available to view in full on the case file and provides explanatory information for the applicant regarding the parameters that will be required when undertaking the future noise assessment to be able to discharge recommended condition 14. It sets out that the noise interval readings undertaken for the validation testing must be every 5 seconds instead of every 3 minutes, with the ventilation strategy operating.  

Amendment to Condition 15 – Sound insulation
The minimum sound performance should be ≥ 48 dB DₙT,w + Ctr, and not a performance of ≥ 53 dB DₙT,w + Ctr, such that the condition should read:
Prior to the commencement of development, full details of the sound insulation performance of the existing and/or proposed separating floor/ceiling construction between the retained ground‑floor commercial use and the first‑floor residential accommodation shall be submitted to and approved in writing by the Local Planning Authority.

The submitted details shall demonstrate, through design calculations and/or manufacturers’ acoustic test data, that the separating floor/ceiling will achieve a minimum airborne sound insulation performance of ≥ 48 dB DₙT,w + Ctr, being at least +5 dB above the minimum standard set out in Approved Document E for separating floors.

The approved sound insulation measures shall be fully installed prior to occupation of the residential units and shall thereafter be retained and maintained for the lifetime of the development.

Reason: To ensure adequate protection of residential amenity from noise associated with the commercial use below, having due regard to policies CS16 and DM10 of the Havant Borough Local Plan (Core Strategy) 2011 and the National planning Policy Framework.  


