Specification of works.
Tree 1: Reduce North East lateral limb by 2 metres or to closest growth point, to achieve 2-metre clearance from building leaving 7 metres remaining. Crown lift to height of 4 metres leaving a remainder of 12 metres canopy height. Remove all deadwood.
Tree 2: Crown lift to height of 3 metres leaving a canopy height of 12 metres remaining. Remove all deadwood.
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